> ## Cross Probing

> Cross probing is the ability to select elements in the schematic and have them mapped to the corresponding components in the layout drawings and vice versa. You can also cross probe between the 2D and 3D view of the same file.

> See Cross Probing Between Two or More EDA Files

> Showing the Net Connectivity when Cross Probing

> Cross Probing Between 2D and 3D Views of the Same File

> Zooming when Cross Probing

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers