> ## Changing the Pen Settings

> With AutoVue, you can specify a thickness for each pen color.

> Note: This option only applies to vector files.

> 1. From the File menu, select Convert.

> The Convert dialog box appears.

> 2. Click Pens.

> The Pen Thickness dialog box appears.

> 3. In the From/To section of the Pen Thickness dialog box, select the Color Index for which you want to modify the thickness.

> Note: To select more than one Color Index, press the Shift or Control keys while selecting.

> 4. From the Units list, select the unit in which you want to set the thickness.
> 5. In the Thickness field, enter a thickness value.
> 6. Press the Enter key.

> The new thickness value appears beside the selected Color Index in the From/To section of the Pen Thickness dialog box.

> 7. To save the changes that you made, click Save As.
>    The Save As dialog box appears.
> 8. Enter a file name for the new pen settings.
> 9. Click OK.

> The new pen settings are saved and appear in the Current Pen Settings list.

> Note: To modify an existing pen setting, select the pen setting from the Current Pen Settings list, make the changes, then click Save.

> 10. Click OK to close the Pen Thickness dialog box.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers