> ## Calibrating an Arc

> 1. Measure an arc in the drawing.

> See Arc in non-Vector Files

> Arc in Vector Files

> 2. From the Arc tab, click Calibrate.

> The Radius Calibration dialog box appears displaying the measured distance.

> 3. From the Measured Radius list, select a unit of measurement to which you want to calibrate the distance.
> 4. Click Calibrate to and enter a value if you want to calibrate to a value.

> Click Set Factor and enter a value if you want to calibrate by a factor.

> 5. Click OK.

> The calibration results appear in the Arc tab.

> 6. Click Close to close the Measurement dialog box.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers