> ## Assigning Pen Settings

> From the Pen Settings tab of the Print Properties dialog box, you can set the thickness of the color indices for the print file.

> Note: AutoVue uses the default pen color indices of the native document for the vector file being viewed. You will not be able to change the color assigned to a pen with AutoVue.

> 1. From the File menu, select Print.

> The Print Properties dialog box appears.

> Note: From the AutoVue toolbar, you can also click Print .

> 2. Click the Pen Settings tab.
> 3. Under From/To, select the Color Index that you want to assign a new pen thickness.

> Note: To change more than one color indices, press the Shift or Control key while selecting.

> 4. From the Units list, select the unit of measure that you want to set the thickness.
> 5. Enter the new thickness.

> The new Thickness appears beside the Color Index.

> 6. In the Print Properties dialog box, configure other print properties
> 7. Configure other print options.

> See Configuring the Print Options

> Setting the Margins

> Adding a Watermark

> Adding a Stamp

> 8. To view a partial view of the file, click Partial Preview.

> The Partial Print Preview dialog box appears.

> See Partial Preview of a File

> 9. Click OK to print.

> The Print dialog box appears indicating the document is printing.

> Note: Pen settings are stored in .c2t files. The Current Pen Settings list displays all existing .c2t files for the current file. The default pen settings are stored in default.c2t and alternate pen settings are stored in alt.c2t.

> See Also Previewing a File Before Printing

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers