Demuxer u16le [PCM unsigned 16-bit little-endian]:
    Common extensions: uw.
u16le demuxer AVOptions:
-sample_rate       <int>        .D....  (from 0 to INT_MAX)
-channels          <int>        .D....  (from 0 to INT_MAX)

