;Windows Modem Setup File
;Copyright (c) 1993-1999 Microsoft Corporation \\MS-IRL\\
;Manufacturer: ZyXEL Comm. Corp.

[Version]
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
DriverVer=07/01/2001,5.1.2535.0
LayoutFile=layout.inf

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%Mfg% = Models
%Hayes% = Hayes
%BT% = BT

[Hayes]
%HT_DSS1.PnP%=HT_DSS1,SERENUM\HAY0AF9

[Models]
%U336E.PnP%=U336E,SERENUM\ZYX0304

; for U-90E modem with firmware version v107 and above
%U90E.PnP%=  U90E, SERENUM\ZYX53FF 
%U90E.PnP%=  U90E, SERENUM\ZYX53FE  
%U90E.PnP%=  U90E, SERENUM\ZYX53FD  
%U90E.PnP%=  U90E, SERENUM\ZYX53FC  
%U90E.PnP%=  U90E, SERENUM\ZYX53FB  
%U90E.PnP%=  U90E, SERENUM\ZYX53FA  
%U90E.PnP%=  U90E, SERENUM\ZYX53F9  
%U90E.PnP%=  U90E, SERENUM\ZYX53F8  
%U90E.PnP%=  U90E, SERENUM\ZYX53F7  
%U90E.PnP%=  U90E, SERENUM\ZYX53F6  
%U90E.PnP%=  U90E, SERENUM\ZYX53F5  
%U90E.PnP%=  U90E, SERENUM\ZYX53F4  
%U90E.PnP%=  U90E, SERENUM\ZYX53F3  
%U90E.PnP%=  U90E, SERENUM\ZYX53F2  
%U90E.PnP%=  U90E, SERENUM\ZYX53F1  
%U90E.PnP%=  U90E, SERENUM\ZYX53F0
%U90E.PnP%=  U90E, SERENUM\ZYX53EF 
%U90E.PnP%=  U90E, SERENUM\ZYX53EE  
%U90E.PnP%=  U90E, SERENUM\ZYX53ED  
%U90E.PnP%=  U90E, SERENUM\ZYX53EC  
%U90E.PnP%=  U90E, SERENUM\ZYX53EB  
%U90E.PnP%=  U90E, SERENUM\ZYX53EA  
%U90E.PnP%=  U90E, SERENUM\ZYX53E9  
%U90E.PnP%=  U90E, SERENUM\ZYX53E8  
%U90E.PnP%=  U90E, SERENUM\ZYX53E7  
%U90E.PnP%=  U90E, SERENUM\ZYX53E6  
%U90E.PnP%=  U90E, SERENUM\ZYX53E5  
%U90E.PnP%=  U90E, SERENUM\ZYX53E4  
%U90E.PnP%=  U90E, SERENUM\ZYX53E3  
%U90E.PnP%=  U90E, SERENUM\ZYX53E2  
%U90E.PnP%=  U90E, SERENUM\ZYX53E1  
%U90E.PnP%=  U90E, SERENUM\ZYX53E0 
%U90E.PnP%=  U90E, SERENUM\ZYX53DF 
%U90E.PnP%=  U90E, SERENUM\ZYX53DE  
%U90E.PnP%=  U90E, SERENUM\ZYX53DD  
%U90E.PnP%=  U90E, SERENUM\ZYX53DC  
%U90E.PnP%=  U90E, SERENUM\ZYX53DB  
%U90E.PnP%=  U90E, SERENUM\ZYX53DA  
%U90E.PnP%=  U90E, SERENUM\ZYX53D9  
%U90E.PnP%=  U90E, SERENUM\ZYX53D8  
%U90E.PnP%=  U90E, SERENUM\ZYX53D7  
%U90E.PnP%=  U90E, SERENUM\ZYX53D6  
%U90E.PnP%=  U90E, SERENUM\ZYX53D5  
%U90E.PnP%=  U90E, SERENUM\ZYX53D4  
%U90E.PnP%=  U90E, SERENUM\ZYX53D3  
%U90E.PnP%=  U90E, SERENUM\ZYX53D2  
%U90E.PnP%=  U90E, SERENUM\ZYX53D1  
%U90E.PnP%=  U90E, SERENUM\ZYX53D0
%U90E.PnP%=  U90E, SERENUM\ZYX5300

%OMNI288S.PnP% = OMNI288S,SERENUM\ZYX0400

; for Omni 288S modem with firmware version v302 and above
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FF  
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FE
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FD
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FC
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FB
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24FA
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F9
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F8
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F7
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F6
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F5
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F4
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F3
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F2
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F1
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24F0
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24EF  
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24EE
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24ED
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24EC
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24EB
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24EA
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E9
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E8
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E7
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E6
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E5
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E4
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E3
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E2
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E1
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24E0
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DF  
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DE
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DD
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DC
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DB
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24DA
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D9
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D8
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D7
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D6
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D5
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D4
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D3
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D2
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D1
%O288S-V90.PnP% = O288S-V90,SERENUM\ZYX24D0


%ZD56.USB%=ZD56, USB\VID_0ACE&PID_1602
	
%E2864I_USA.PnP% =E2864I_USA,SERENUM\ZYX02FF
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02FE
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02FD
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02FC
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02FB
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02FA
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F9
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F8
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F7
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F6
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F5
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F4
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F3
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F2
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F1
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02F0
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02EF
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02EE
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02ED
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02EC
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02EB
%E2864I_JPN.PnP%=E2864I_JPN,SERENUM\ZYX02EA
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E9
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E8
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E7
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E6
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E5
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E4
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E3
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E2
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E1
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02E0
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DF
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DE
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DD
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DC
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DB
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02DA
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02D9
%E2864I_DSS1.PnP%=E2864I_DSS1,SERENUM\ZYX02D8
%E2864I_1TR6.PnP%=E2864I_1TR6,SERENUM\ZYX0200

%E2864V90.PnP%=E2864V90,SERENUM\zyx21FF

%E2864V90.PnP%=E2864V90,SERENUM\ZYX21FE
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21FD
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21FC
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21FB
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21FA
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F9
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F8
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F7
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F6
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F5
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F4
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F3
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F2
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F1
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21F0
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21EF
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21EE
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21ED
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21EC
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21EB
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21EA
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E9
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E8
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E7
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E6
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E5
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E4
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E3
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E2
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E1
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21E0
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DF
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DE
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DD
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DC
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DB
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21DA
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21D9
%E2864V90.PnP%=E2864V90,SERENUM\ZYX21D8
%E2864V90.PnP%=E2864V90,SERENUM\ZYX2100
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FF
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FE
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FD
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FC
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FB
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01FA
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F9
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F8
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F7
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F6
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F5
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F4
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F3
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F2
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F1
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01F0
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01EF
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01EE
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01ED
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01EC
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01EB
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01EA
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E9
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E8
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E7
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E6
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E5
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E4
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E3
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E2
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E1
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01E0
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DF
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DE
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DD
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DC
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DB
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01DA
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D9
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D8
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D7
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D6
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D5
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D4
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D3
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D2
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D1
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01D0
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CF
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CE
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CD
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CC
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CB
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01CA
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C9
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C8
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C7
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C6
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C5
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C4
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C3
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C2
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C1
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01C0
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BF
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BE
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BD
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BC
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BB
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01BA
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B9
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B8
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B7
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B6
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B5
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B4
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B3
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B2
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B1
%E2864V34.PnP%=E2864V34,SERENUM\ZYX01B0
%E2864V34.PnP%=E2864V34, SERENUM\ZYX0100

%E2864I-V90_USA.PnP% =E2864I-V90_USA, SERENUM\ZYX32FF
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32FE
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32FD
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32FC
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32FB
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32FA
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F9
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F8
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F7
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F6
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F5
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F4
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F3
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F2
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F1
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32F0
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32EF
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32EE
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32ED
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32EC
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32EB
%E2864I-V90_JAPAN.PnP%=E2864I-V90_JAPAN,SERENUM\ZYX32EA
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E9
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E8
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E7
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E6
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E5
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E4
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E3
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E2
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E1
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32E0
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DF
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DE
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DD
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DC
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DB
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32DA
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D9
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D8
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D7
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D6
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D5
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D4
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D3
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D2
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D1
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32D0

%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CF
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CE
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CD
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CC
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CB
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32CA
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C9
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C8
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C7
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C6
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C5
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C4
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C3
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C2
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C1
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32C0
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BF
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BE
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BD
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BC
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BB
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32BA
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B9
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B8
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B7
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B6
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B5
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B4
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B3
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B2
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B1
%E2864I-V90_DSS1.PnP%=E2864I-V90_DSS1,SERENUM\ZYX32B0

%OT_USA.PnP%= OT_USA,SERENUM\ZYX09FF
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09FE
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09FD
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09FC
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09FB
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09FA
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F9
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F8
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F7
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F6
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F5
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F4
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F3
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F2
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F1
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09F0
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09EF
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09EE
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09ED
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09EC
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09EB
%OT_JPN.PnP%=OT_JPN,SERENUM\ZYX09EA
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E9
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E8
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E7
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E6
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E5
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E4
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E3
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E2
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E1
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09E0
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DF
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DE
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DD
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DC
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DB
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09DA
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D9
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D8
%OT_1TR6.PnP%=OT_1TR6,SERENUM\ZYX0900

%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D7
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D6
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D5
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D4
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D3
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D2
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D1
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09D0
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CF
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CE
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CD
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CC
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CB
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09CA
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C9
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C8
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C7
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C6
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C5
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C4
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C3
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C2
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C1
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09C0
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BF
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BE
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BD
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BC
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BB
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09BA
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B9
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B8
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B7
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B6
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B5
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B4
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B3
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B2
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B1
%OT_DSS1.PnP%=OT_DSS1,SERENUM\ZYX09B0

  
%OD_USA.PnP%= OD_USA,SERENUM\ZYX0CFF
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CFE
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CFD
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CFC
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CFB
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CFA
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF9
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF8
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF7
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF6
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF5
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF4
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF3
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF2
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF1
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CF0
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CEF
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CEE
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CED
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CEC
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CEB
%OD_JPN.PnP% =OD_JPN,SERENUM\ZYX0CEA
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE9
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE8
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE7
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE6
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE5
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE4
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE3
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE2
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE1
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CE0
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDF
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDE
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDD
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDC
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDB
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CDA
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CD9
%OD_DSS1.PnP%=OD_DSS1,SERENUM\ZYX0CD8
%OD_1TR6.PnP%=OD_1TR6,SERENUM\ZYX0C00

; omni.net LCD Plus
%OLP_USA.PnP%= OLP_USA, SERENUM\ZYX0FFF
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FFE
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FFD
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FFC
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FFB
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FFA
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF9
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF8
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF7
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF6
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF5
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF4
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF3
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF2
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF1
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FF0
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FEF
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FEE
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FED
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FEC
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FEB
%OLP_JAPAN.PnP%=OLP_JAPAN,SERENUM\ZYX0FEA
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE9
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE8
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE7
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE6
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE5
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE4
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE3
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE2
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE1
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FE0
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDF
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDE
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDD
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDC
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDB
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FDA
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD9
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD8
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD7
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD6
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD5
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD4
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD3
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD2
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD1
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FD0
%OLP_DSS1.PnP%=OLP_DSS1,SERENUM\ZYX0FCF

%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DFE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DFD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DFC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DFB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DFA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DF0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DEF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DEE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DED
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DEC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DEB
%OL_JPN.PnP%=OL_JPN,SERENUM\ZYX0DEA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DE0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DDA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DD0



%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DCA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DC0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DBA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0DB0

%OP_USA.PnP%= OP_USA,SERENUM\ZYX0BFF
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BFE
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BFD
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BFC
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BFB
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BFA
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF9
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF8
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF7
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF6
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF5
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF4
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF3
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF2
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF1
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BF0
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BEF
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BEE
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BED
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BEC
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BEB
%OP_JPN.PnP%=OP_JPN,SERENUM\ZYX0BEA
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE9
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE8
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE7
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE6
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE5
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE4
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE3
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE2
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE1
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BE0
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDF
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDE
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDD
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDC
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDB
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BDA
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD9
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD8
%OP_1TR6.PnP%=OP_1TR6,SERENUM\ZYX0B00

; omni.net
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AFE
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AFD
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AFC
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AFB
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AFA
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF9
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF8
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF7
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF6
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF5
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF4
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF3
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF2
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF1
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AF0
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AEF
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AEE
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AED
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AEC
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AEB
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AEA
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE9
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE8
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE7
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE6
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE5
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE4
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE3
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE2
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE1
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AE0
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADF
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADE
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADD
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADC
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADB
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0ADA
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD9
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD8
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD7
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD6
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD5
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD4
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD3
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD2
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD1
%ON_DSS1.PnP%=ON_DSS1,SERENUM\ZYX0AD0
;%ON_1TR6.PnP%=ON_1TR6,SERENUM\ZYX0A00



%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD7
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD6
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD5
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD4
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD3
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD2
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD1
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BD0
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCF
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCE
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCD
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCC
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCB
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BCA
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC9
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC8
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC7
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC6
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC5
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC4
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC3
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC2
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC1
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BC0
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBF
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBE
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBD
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBC
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBB
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BBA
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB9
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB8
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB7
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB6
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB5
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB4
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB3
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB2
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB1
%OP_DSS1.PnP%=OP_DSS1,SERENUM\ZYX0BB0


%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EFE
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EFD
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EFC
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EFB
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EFA
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF9
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF8
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF7
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF6
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF5
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF4
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF3
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF2
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF1
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EF0
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EEF
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EEE
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EED
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EEC
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EEB
%OLM_JAPAN.PnP%=OLM_JAPAN,SERENUM\ZYX0EEA
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE9
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE8
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE7
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE6
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE5
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE4
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE3
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE2
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE1
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EE0
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EDF
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EDE
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EDD
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EDC
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EDB
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED8
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED7
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED6
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED5
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED4
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED3
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED2
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED1
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ED0

;more than released
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECF
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECE
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECD
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECC
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECB
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0ECA
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC9
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC8
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC7
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC6
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC5
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC4
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC3
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC2
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC1
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EC0
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBF
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBE
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBD
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBC
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBB
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EBA
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB9
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB8
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB7
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB6
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB5
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB4
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB3
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB2
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB1
%OLM_DSS1.PnP%=OLM_DSS1,SERENUM\ZYX0EB0

%OM90.PnP%=OM90,SERENUM\ZYX55FF
%OM90.PnP%=OM90,SERENUM\ZYX55FE
%OM90.PnP%=OM90,SERENUM\ZYX55FD
%OM90.PnP%=OM90,SERENUM\ZYX55FC
%OM90.PnP%=OM90,SERENUM\ZYX55FB
%OM90.PnP%=OM90,SERENUM\ZYX55FA
%OM90.PnP%=OM90,SERENUM\ZYX55F9
%OM90.PnP%=OM90,SERENUM\ZYX55F8
%OM90.PnP%=OM90,SERENUM\ZYX55F7
%OM90.PnP%=OM90,SERENUM\ZYX55F6
%OM90.PnP%=OM90,SERENUM\ZYX55F5
%OM90.PnP%=OM90,SERENUM\ZYX55F4
%OM90.PnP%=OM90,SERENUM\ZYX55F3
%OM90.PnP%=OM90,SERENUM\ZYX55F2
%OM90.PnP%=OM90,SERENUM\ZYX55F1
%OM90.PnP%=OM90,SERENUM\ZYX55F0
%OM90.PnP%=OM90,SERENUM\ZYX55EF
%OM90.PnP%=OM90,SERENUM\ZYX55EE
%OM90.PnP%=OM90,SERENUM\ZYX55ED
%OM90.PnP%=OM90,SERENUM\ZYX55EC
%OM90.PnP%=OM90,SERENUM\ZYX55EB
%OM90.PnP%=OM90,SERENUM\ZYX55EA
%OM90.PnP%=OM90,SERENUM\ZYX55E9
%OM90.PnP%=OM90,SERENUM\ZYX55E8
%OM90.PnP%=OM90,SERENUM\ZYX55E7
%OM90.PnP%=OM90,SERENUM\ZYX55E6
%OM90.PnP%=OM90,SERENUM\ZYX55E5
%OM90.PnP%=OM90,SERENUM\ZYX55E4
%OM90.PnP%=OM90,SERENUM\ZYX55E3
%OM90.PnP%=OM90,SERENUM\ZYX55E2
%OM90.PnP%=OM90,SERENUM\ZYX55E1
%OM90.PnP%=OM90,SERENUM\ZYX55E0
%OM90.PnP%=OM90,SERENUM\ZYX55DF
%OM90.PnP%=OM90,SERENUM\ZYX55DE
%OM90.PnP%=OM90,SERENUM\ZYX55DD
%OM90.PnP%=OM90,SERENUM\ZYX55DC
%OM90.PnP%=OM90,SERENUM\ZYX55DB
%OM90.PnP%=OM90,SERENUM\ZYX55DA
%OM90.PnP%=OM90,SERENUM\ZYX55D9
%OM90.PnP%=OM90,SERENUM\ZYX55D8
%OM90.PnP%=OM90,SERENUM\ZYX55D7
%OM90.PnP%=OM90,SERENUM\ZYX55D6
%OM90.PnP%=OM90,SERENUM\ZYX55D5
%OM90.PnP%=OM90,SERENUM\ZYX55D4
%OM90.PnP%=OM90,SERENUM\ZYX55D3
%OM90.PnP%=OM90,SERENUM\ZYX55D2
%OM90.PnP%=OM90,SERENUM\ZYX55D1
%OM90.PnP%=OM90,SERENUM\ZYX55D0


;removed some ids as wont be released
[BT]
%IP_DSS1.PnP%=IP_DSS1,SERENUM\ZYX11F9
%IP_DSS1.PnP%=IP_DSS1,SERENUM\ZYX1155



[Strings]
MSFT= "Microsoft"
Hayes= "Hayes"
BT = "British Telecom"
Mfg="ZyXEL Communications Corp"

IP_DSS1.PnP	= "BT Ignition Pro (Serial only), PnP"

OLM_DSS1	= "ZyXEL omni.net LCD+M (DSS1)"
OLM_DSS1.PnP	= "ZyXEL omni.net LCD+M (DSS1), PnP"
OLM_JAPAN	= "ZyXEL omni.net LCD+M (Japan)"
OLM_JAPAN.PnP	= "ZyXEL omni.net LCD+M (Japan), PnP"

OM90.PnP        = "ZyXEL Omni56K, Plug&Play"
ZD56.USB        = "ZyXEL Omni 56K USB Modem"
USBFilterString = "ZyXEL Omni 56K USB Modem Driver"
OLP_DSS1.PnP	= "ZyXEL omni.net LCD Plus (Serial only, DSS1), Plug&Play"
OLP_JAPAN.PnP	= "ZyXEL omni.net LCD Plus (Serial only, Japan), Plug&Play"
OLP_USA.PnP	= "ZyXEL omni.net LCD Plus (Serial only, USA), Plug&Play"
ON_DSS1.PnP="ZyXEL omni.net (DSS1), PnP"
OD_DSS1.PnP="ZyXEL omni.net D (DSS1), PnP"
OD_1TR6.PnP="ZyXEL omni.net D (1TR6), PnP"
OD_USA.PnP="ZyXEL omni.net D (USA), PnP"
OD_JPN.PnP="ZyXEL omni.net D (Japan), PnP"
OL_DSS1.PnP="ZyXEL omni.net LCD (DSS1), PnP"
OL_JPN.PnP="ZyXEL omni.net LCD (Japan), PnP"
OP_DSS1.PnP="ZyXEL omni.net PLUS (DSS1), PnP"
OP_1TR6.PnP="ZyXEL omni.net PLUS (1TR6), PnP"
OP_USA.PnP="ZyXEL omni.net PLUS (USA), PnP"
OP_JPN.PnP="ZyXEL omni.net PLUS (Japan), PnP"
OT_DSS1.PnP="ZyXEL Omni TA128 (DSS1), PnP"
OT_1TR6.PnP="ZyXEL Omni TA128 (1TR6), PnP"
OT_USA.PnP="ZyXEL Omni TA128 (USA), PnP"
OT_JPN.PnP="ZyXEL Omni TA128 (Japan), PnP"
E2864I_DSS1.PnP="ZyXEL Elite 2864I ISDN (DSS1) Modem(V.34)+Fax, PnP"
E2864I_USA.PnP="ZyXEL Elite 2864I ISDN (USA) Modem(V.34)+Fax, PnP"
E2864I_1TR6.PnP="ZyXEL Elite 2864I ISDN (1TR6) Modem(V.34)+Fax, PnP"
E2864I_JPN.PnP="ZyXEL Elite 2864I ISDN (Japan) Modem(V.34)+Fax, PnP"
HT_DSS1.PnP="Accura ISDN DSS1 PnP"
OMNI288S.PnP="ZyXEL Omni 288S Modem(V.34)+Fax, PnP"
O288S-V90.PnP="ZyXEL Omni 288S Modem(V.90)+Fax, PnP"
U336E.PnP= "ZyXEL U-336E Modem(V.34)+Fax, PnP"
U90E.PnP = "ZyXEL U-90E Modem(V.90)+Fax, PnP"
E2864V90.PnP="ZyXEL Elite 2864 Modem(V.90)+Fax, PnP"
E2864V34.PnP="ZyXEL Elite 2864 Modem(V.34)+Fax, PnP"
E2864I-V90_DSS1.PnP  = "ZyXEL Elite 2864I Modem(V.90)+Fax (DSS1), Plug&Play"
E2864I-V90_JAPAN.PnP = "ZyXEL Elite 2864I Modem(V.90)+Fax (Japan), Plug&Play"
E2864I-V90_USA.PnP   = "ZyXEL Elite 2864I Modem(V.90)+Fax (USA), Plug&Play"

[IP_DSS1]
DriverVer=04/03/2001,5.00.2462.0
include=mdmgl008.inf 
AddReg=All, MDMGL008.ALL, INIT.DSS1, OLP.Data, OL.Responses, ISDNOLP.All, ISDN.DSS1

[OM90]
AddReg=All, Mfg.AddReg, OM90.Fax, OM90.Voice, OM90.Responses, OM90.AddReg

[ZD56.NT]
DriverVer=02/22/2001,5.00.2442.1
CopyFiles=FakeModemCopyFileSection
AddReg=All, Mfg.AddReg, OM90.Fax, OM90.voice, OM90.Responses, ZD56.AddReg

[OLM_DSS1]
DriverVer=04/04/2001,5.00.2463.1
include=mdmgl008.inf
AddReg=All, MDMGL008.ALL, OLP.Data, OLM.Responses,  OLM.Fax, ISDNON.All, ISDN.DSS1, OLM.AddReg

[OLM_JAPAN]
DriverVer=04/04/2001,5.00.2463.1
include=mdmgl008.inf
AddReg=All, MDMGL008.ALL, OLP.Data, OLM.Responses,  OLM.Fax, ISDNON.All, ISDN.JAPAN, OLM.AddReg

[OLP_USA]
DriverVer=04/03/2001,5.00.2462.0
include=mdmgl008.inf
AddReg=All, MDMGL008.ALL, OLP.Data, OL.Responses, ISDNOLP.All, ISDN.USA

[OLP_DSS1]
DriverVer=04/03/2001,5.00.2463.0
include=mdmgl008.inf
AddReg=All, MDMGL008.ALL, INIT.DSS1, OLP.Data, OL.Responses, ISDNOLP.All, ISDN.DSS1

[OLP_JAPAN]
DriverVer=04/03/2001,5.00.2462.0
include=mdmgl008.inf
AddReg=All, MDMGL008.ALL, OLP.Data, OL.Responses, ISDNOLP.All, ISDN.JAPAN


[E2864I-V90_DSS1]
DriverVer=12/06/2000,5.00.2403.0
include=mdmgl008.inf, mdmgl006.inf
AddReg=All, MDMGL008.ALL, E2864I.Data, E2864V90.Fax, E2864I.Responses, MDMGL006.Common, MDMGL008.ISDN, Additional.Responses, ISDNON.All, ISDN.DSS1, E2864I.AddReg

[E2864I-V90_JAPAN]
DriverVer=12/06/2000,5.00.2403.0
include=mdmgl008.inf, mdmgl006.inf
AddReg=All, MDMGL008.ALL, E2864I.Data, E2864V90.Fax, E2864I.Responses, MDMGL006.Common, MDMGL008.ISDN, Additional.Responses,ISDNON.All, ISDN.JAPAN, E2864I.AddReg

[E2864I-V90_USA]
DriverVer=12/06/2000,5.00.2403.0
include=mdmgl008.inf, mdmgl006.inf
AddReg=All, MDMGL008.ALL, E2864I.Data, E2864V90.Fax, E2864I.Responses, MDMGL006.Common, MDMGL008.ISDN, Additional.Responses, ISDNON.All, ISDN.USA, E2864I.AddReg

[E2864V34]
include=mdmgl008.inf, mdmgl006.inf
DriverVer=12/06/2000,5.00.2403.0
AddReg=All, Mfg.AddReg, E2864V34.AddReg, E2864V90.Fax, E2864.voice, E2864I.Responses, MDMGL006.Common, MDMGL008.ALL

[E2864V90]
include=mdmgl006.inf, mdmgl008.inf
DriverVer=12/06/2000,5.00.2403.0
AddReg=All, Mfg.AddReg, E2864V90.AddReg, E2864V90.Fax, Fax2DRAM, E2864I.Responses, MDMGL006.Common, MDMGL008.ALL


[U336E]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,Mfg.AddReg,U336E.AddReg,MDMGL008.ALL,E2864I.Responses, OM90.Voice, OM90.Fax

[U90E]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,Mfg.AddReg,U336E.AddReg,MDMGL008.ALL,E2864I.Responses, OM90.Voice, OM90.Fax

[OMNI288S]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,Mfg.AddReg,OMNI288S.AddReg,MDMGL008.ALL,E2864I.Responses

[O288S-V90]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,Mfg.AddReg,OMNI288S.AddReg,MDMGL008.ALL,E2864I.Responses

[HT_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNHT.All,ISDNT.DSS1

[ON_DSS1]	;Latest Omni.net rev 1.20
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNON.All,ISDNT.DSS1

[OP_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OP.Data,MDMGL008.ISDN,ISDNOP.All,ISDNOP.DSS1

[OP_1TR6]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl008.inf
AddReg=All,MDMGL008.ALL,OP.Data,MDMGL008.ISDN,ISDNOP.All,ISDNOP.1TR6

[OP_USA]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OP.Data,MDMGL008.ISDN,ISDNOP.All,ISDNOP.USA,MDMGL008.US

[OP_JPN]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OP.Data,MDMGL008.ISDN,ISDNOP.All,ISDNOP.JPN

[OD_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OD.Data,MDMGL008.ISDN,ISDNOD.All,ISDNOD.DSS1

[OD_1TR6]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OD.Data,MDMGL008.ISDN,ISDNOD.All,ISDNOD.1TR6

[OD_USA]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OD.Data,MDMGL008.ISDN,ISDNOD.All,ISDNOD.USA,MDMGL008.US

[OD_JPN]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OD.Data,MDMGL008.ISDN,ISDNOD.All,ISDNOD.JPN

[OL_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OL.Data,MDMGL008.ISDN,ISDNOL.All,ISDNOL.DSS1

[OL_JPN]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OL.Data,MDMGL008.ISDN,ISDNOL.All,ISDNOL.JPN

[OT_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNOP.All,ISDNT.DSS1

[OT_1TR6]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNOP.All,ISDNT.1TR6

[OT_USA]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNOP.All,ISDNT.USA,MDMGL008.US

[OT_JPN]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,OT.Data,MDMGL008.ISDN,ISDNOP.All,ISDNT.JPN

[E2864I_DSS1]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,E2864I.Data,E2864I.Responses,ISDNE.All,ISDNE.DSS1

[E2864I_USA]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,E2864I.Data,E2864I.Responses,ISDNE.All,ISDNE.USA,MDMGL008.US

[E2864I_1TR6]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,E2864I.Data,E2864I.Responses,ISDNE.All,ISDNE.1TR6

[E2864I_JPN]
include=mdmgl008.inf
DriverVer=06/01/1999,5.00.0000.0
AddReg=All,MDMGL008.ALL,E2864I.Data,E2864I.Responses,ISDNE.All,ISDNE.JPN

[All]
HKR,,DeviceType,1,01
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Responses, "<cr><lf>FM:",                             1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>TO:",                             1, 96, 00, 00,00,00,00, 00,00,00,00

[OM90.AddReg]
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 7f,07,00,00, 00,08,07,00, C0,DA,00,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR, Init,      1,,                                        "AT&FE0X4<cr>"
HKR, Init, 3,, "AT<CR>"
HKR, Hangup,    1,,                                        "ATH0E1<cr>"
HKR, K56mode,   1,,                                        "AT<cr>"
HKR, Settings, SpeakerVolume_High,,                        "L6"


[ZD56.AddReg]
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 7f,07,00,00, 00,08,07,00, C0,DA,00,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, Reset,,                                              "ATZ<cr>"
HKR, Init,      1,,                                        "AT&FE0X4<cr>"
HKR,,VoiceProfile,                      1,23,30,01,02
HKR,,HandsetCloseDelay,                 1,01,00,00,00
              
[OLM.AddReg]
HKR, EnableCallerID,1,,                     "ATS84.4=0<cr>"
HKR, ISDN\Init,1,,                          "AT&O1<cr>"
HKR, Init,      5,,                                        "ATCN<0><cr>"
HKR, Init,      6,,                                        "ATCI<00><cr>"
HKR, ISDN\NvSave,2,,                        "AT<cr>"

[E2864I.AddReg]
HKR,, Properties, 1, 00,00,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 07,00,00,00, 73,05,00,00, 00,08,07,00, 00,f4,01,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, Reset,, "ATZ<cr>"
HKR, Init,      1,, "AT&FZE0X8<cr>"
HKR, Init,      2,, "ATV1&D3&C1S0=0<cr>"
HKR, Init,      3,, "AT&L1S38.3=1S48.2=1<cr>"
HKR, Init,      4,, "ATS84.4=1S118.3=1<cr>"
HKR, Init,      5,, "ATCN<0><cr>"
HKR, Init,      6,, "ATCI<00><cr>"
HKR, EnableCallerID,1,,  "ATS84.4=0<cr>"
HKR, ISDN\Init,1,,    "AT&O1<cr>"
HKR, ISDN\NvSave,2,,  "AT<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "ATB01&J0&E0S80.6=1<cr>"


[E2864V34.AddReg]
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 7f,07,00,00, 00,08,07,00, C0,DA,00,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, Reset,,  "ATZ<cr>"
HKR, Init,      1,, "AT&FE0X6<cr>"
HKR, Init,      2,, "ATV1&D3&C1S0=0<cr>"
HKR, Init,      3,, "ATS11=90S48.2=1<cr>"
HKR, Hangup,    2,, "ATZ<cr>"
HKR, K56mode,   1,, "AT<cr>"
HKR, V90mode,   1,, "AT<cr>"
HKR, Settings, Compression_Off,, "&K0"

[E2864V90.AddReg]
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 7f,07,00,00, 00,08,07,00, C0,DA,00,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR, Init,      1,, "AT&FE0X6<cr>"
HKR, Init,      2,, "ATV1&D3&C1S0=0<cr>"
HKR, Init,      3,, "ATS11=90S48.2=1<cr>"
HKR, Hangup,    2,, "ATZ<cr>"
HKR, K56mode,   1,, "AT<cr>"
HKR, Settings, Compression_Off,, "&K0"
HKR, Responses, "<cr><lf>COMPRESSION: None<cr><lf>",       	1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: MNP5<cr><lf>",       	1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: V42b<cr><lf>",       	1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: None<cr><lf>",          	1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: MNP4<cr><lf>",         	1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V42<cr><lf>",           	1, 01, 02, 00,00,00,00, 00,00,00,00

[U336E.AddReg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,7F,07,00,00,00,C2,01,00,40,83,00,00
HKR,Init,1,,"AT&FE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"ATS11=90S57.4=1<cr>"

[OMNI288S.AddReg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,7F,07,00,00,00,C2,01,00,40,83,00,00
HKR,Init,1,,"AT&FE0X7<cr>"
HKR,Init,2,,"ATS11=90S57.4=1<cr>"
HKR,Settings,Pulse,,"P"
HKR,Settings,Tone,,"T"
HKR,Settings,Blind_Off,,"S41.4=0"
HKR,Settings,Blind_On,,"S41.4=1"
HKR,Settings,Modulation_CCITT,,"B0"
HKR,Settings,Modulation_Bell,,"B1"
HKR,Settings,ErrorControl_Cellular,,"S43.3=0S57.5=1&K3*E0"
HKR,Settings,ErrorControl_Cellular_Forced,,"S43.3=0S57.5=1&K3*E1"

[INIT.DSS1]
HKR, Init,      5,,  "ATCN<0><cr>"
HKR, Init,      6,,  "ATCI<00><cr>"

[ISDNE.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"AT&O2B40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"AT&O2B40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "AT&O2B40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "AT&O2B40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "AT&O2B40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"AT&O2B40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"AT&O2B40&J3&E0S87.2=0S118.3=1<cr>"
HKR,Protocol\ISDN\V120_56K ,1,,"AT&O2B20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "AT&O2B20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "AT&O2B20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"AT&O2B20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"AT&O2B00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "AT&O2B00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "AT&O2B01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"AT&O2B04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_2DOT4K,1,, "AT&O2B13S80.6=1<cr>"
HKR,Protocol\ISDN\V110_4DOT8K,1,, "AT&O2B14S80.6=1<cr>"
HKR,Protocol\ISDN\V110_9DOT6K,1,, "AT&O2B15S80.6=1<cr>"
HKR,Protocol\ISDN\V110_14DOT4K,1,,"AT&O2B16S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"AT&O2B17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,,"AT&O2B18<cr>"
HKR,Protocol\ISDN\ANALOG_V34,1,, "AT&O0<cr>"

[ISDNE.USA]
HKR,ISDN\SwitchType,SWITCH_DMS100,,"ATP0<cr>"   
HKR,ISDN\SwitchType,SWITCH_NI1,,"ATP2<cr>"   
HKR,ISDN\SwitchType,SWITCH_ATT1,, "ATP6<cr>"   
HKR,ISDN,CompatibilityFlags, 1,00,00,00,01
HKR,ISDN\SetSpid,1,,"ATSPID0=%s<cr>"
HKR,ISDN\SetSpid,2,,"ATSPID1=%s<cr>"
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  
HKR,ISDN\NvSave,2,,"ATZ<cr>"

[ISDNE.1TR6]
HKR,ISDN\SwitchType,SWITCH_1TR6,, "AT<cr>"
HKR,ISDN\SetEAZ,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetEAZ,2 ,,"AT&ZI7=%s<cr>"  
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  

[ISDNE.DSS1]
HKR,ISDN\SwitchType,SWITCH_DSS1,, "AT<cr>"
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  

[ISDNE.JPN]
HKR,ISDN\SwitchType,SWITCH_INS64,,"AT<cr>"   
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  
HKR,Protocol\ISDN\V110_57DOT6K,1,, "AT&O2B19<cr>"

[Mfg.AddReg]
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"ATS11=90S57.4=1<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATA<cr>"
HKR,Settings,Blind_Off,,"S41.4=0"
HKR,Settings,Blind_On,,"S41.4=1"
HKR,Settings,CallSetupFailTimer,,"S7=<#>"
HKR,Settings,Compression_On,, "&K4"
HKR,Settings,Compression_Off,,"S127=0"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,ErrorControl_Cellular,,"S43.3=0S57.5=1&K3*E0"
HKR,Settings,ErrorControl_Cellular_Forced,,"S43.3=0S57.5=1&K3*E1"
HKR,Settings,ErrorControl_Forced,,"&K3*E1"
HKR,Settings,ErrorControl_Off,,"&K0"
HKR,Settings,ErrorControl_On,,"&K3*E0"
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Modulation_CCITT,,"B0"
HKR,Settings,Modulation_Bell,, "B1"
HKR,Settings,Modulation_CCITT_V23,, "&N12"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,,"P"
HKR,Settings,SpeakerMode_Dial,,"M1"
HKR,Settings,SpeakerMode_Off,,"M0"
HKR,Settings,SpeakerMode_On,,"M2"
HKR,Settings,SpeakerMode_Setup,,"M3"
HKR,Settings,SpeakerVolume_High,,"L7"
HKR,Settings,SpeakerVolume_Low,,"L1"
HKR,Settings,SpeakerVolume_Med,,"L4"
HKR,Settings,SpeedNegotiation_Off,,""
HKR,Settings,SpeedNegotiation_On,,"&N0"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"
HKR,Responses,"0<cr>", 1,00,00,00,00,00,00,00,00,00,00 
HKR,Responses,"9<cr>", 1,01,00,00,00,00,00,00,00,00,00 
HKR,Responses,"1<cr>", 1,02,00,00,00,00,00,00,00,00,00 
HKR,Responses,"4<cr>", 1,03,00,00,00,00,00,00,00,00,00 
HKR,Responses,"3<cr>", 1,04,00,00,00,00,00,00,00,00,00 
HKR,Responses,"6<cr>", 1,05,00,00,00,00,00,00,00,00,00 
HKR,Responses,"7<cr>", 1,06,00,00,00,00,00,00,00,00,00 
HKR,Responses,"8<cr>", 1,07,00,00,00,00,00,00,00,00,00 
HKR,Responses,"2<cr>", 1,08,00,00,00,00,00,00,00,00,00 
HKR,Responses,"<cr><lf>OK<cr><lf>", 1,00,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RINGING<cr><lf>", 1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT<cr><lf>", 1,02,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>ERROR<cr><lf>", 1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO CARRIER<cr><lf>",1,04,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO DIALTONE<cr><lf>", 1,05,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>BUSY<cr><lf>",  1,06,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO ANSWER<cr><lf>", 1,07,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING<cr><lf>",  1,08,00,00,00,00,00,00,00,00,00

[E2864I.Data]
HKR,,Properties,1,00,00,00,00,ff,00,00,00,ff,00,00,00,07,00,00,00,07,00,00,00,73,05,00,00,00,08,07,00,00,f4,01,00
HKR,,DCB, 1,1c,00,00,00,00,c2,01,00,15,20,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FZE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"ATS38.3=1<cr>"
HKR,Init,4,,"AT&L1S48.2=1<cr>"
HKR,Init,5,,"ATS84.4=1<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATA<cr>"
HKR,Settings,Blind_Off,,""
HKR,Settings,CallSetupFailTimer,, "S7=<#>"
HKR,Settings,Compression_Off,,"&K00"
HKR,Settings,Compression_On,, "&K4&K44"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,ErrorControl_Off,,"&K0"
HKR,Settings,ErrorControl_On,,"&K3*E0"
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Modulation_Bell,,"B1"
HKR,Settings,Modulation_CCITT,,"B0"
HKR,Settings,Modulation_CCITT_V23,, "&N12&O0"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,, "P"
HKR,Settings,SpeakerMode_Dial,,"M1"
HKR,Settings,SpeakerMode_Off,,"M0"
HKR,Settings,SpeakerMode_On,, "M2"
HKR,Settings,SpeakerMode_Setup,,"M3"
HKR,Settings,SpeakerVolume_High,, "L7"
HKR,Settings,SpeakerVolume_Low,,"L1"
HKR,Settings,SpeakerVolume_Med,,"L4"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"

[ISDNOD.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\AUTO_1CH,1,, "ATB95&J0S80.6=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"ATB40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"ATB40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "ATB40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "ATB40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"ATB40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"
HKR,Protocol\ISDN\V120_56K ,1,,"ATB20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "ATB20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "ATB20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"ATB20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"ATB00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "ATB01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"ATB04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_2DOT4K,1,, "ATB13S80.6=1<cr>"
HKR,Protocol\ISDN\V110_4DOT8K,1,, "ATB14S80.6=1<cr>"
HKR,Protocol\ISDN\V110_9DOT6K,1,, "ATB15S80.6=1<cr>"
HKR,Protocol\ISDN\V110_14DOT4K,1,,"ATB16S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"ATB17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,,"ATB18<cr>"

[ISDNOD.USA]
HKR,ISDN\SwitchType,SWITCH_DMS100,,"ATP0<cr>"   
HKR,ISDN\SwitchType,SWITCH_NI1,,"ATP2<cr>"   
HKR,ISDN\SwitchType,SWITCH_ATT1,, "ATP6<cr>"   
HKR,ISDN,CompatibilityFlags, 1,00,00,00,01
HKR,ISDN\SetSpid,1,,"ATSPID0=%s<cr>"
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\NvSave,2,,"ATZ<cr>"

[ISDNOD.1TR6]
HKR,ISDN\SwitchType,SWITCH_1TR6,, "AT<cr>"
HKR,ISDN\SetEAZ,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  

[ISDNOD.DSS1]
HKR,ISDN\SwitchType,SWITCH_DSS1,, "AT<cr>"
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  

[ISDNOD.JPN]
HKR,ISDN\SwitchType,SWITCH_INS64,,"AT<cr>"   
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,Protocol\ISDN\V110_57DOT6K,1,, "AT&O1B19<cr>"

[OD.Data]
HKR,,Properties,1,00,00,00,00,ff,00,00,00,ff,00,00,00,00,00,00,00,00,00,00,00,31,01,00,00,00,08,07,00,00,f4,01,00
HKR,,DCB, 1,1c,00,00,00,00,c2,01,00,15,20,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FZE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"ATS38.3=1<cr>"
HKR,Init,4,,"ATS84.4=1S118.3=1&K3<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATA<cr>"
HKR,Settings,CallSetupFailTimer,, "S7=<#>"
HKR,Settings,Compression_Off,,"&K00"
HKR,Settings,Compression_On,, "&K44"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,ErrorControl_Off,,"&K0"
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,, "P"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"

[ISDNOL.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\Init,2,,"ATCN<0><cr>"
HKR,ISDN\Init,3,,"ATCI<00><cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\AUTO_1CH,1,, "AT&O2B95&J0S80.6=0S84.4=1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"AT&O2B40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"AT&O2B40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "AT&O2B40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "AT&O2B40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "AT&O2B40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"AT&O2B40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"
HKR,Protocol\ISDN\V120_56K,1,, "AT&O2B20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "AT&O2B20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "AT&O2B20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"AT&O2B20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"AT&O2B00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "AT&O2B00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "AT&O2B01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"AT&O2B04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_2DOT4K,1,, "AT&O2B13S80.6=1<cr>"
HKR,Protocol\ISDN\V110_4DOT8K,1,, "AT&O2B14S80.6=1<cr>"
HKR,Protocol\ISDN\V110_9DOT6K,1,, "AT&O2B15S80.6=1<cr>"
HKR,Protocol\ISDN\V110_14DOT4K,1,,"AT&O2B16S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"AT&O2B17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,,"AT&O2B18<cr>"

[ISDNOL.DSS1]
HKR,ISDN\SwitchType,SWITCH_DSS1,, "AT<cr>"
HKR,ISDN\SetMSN,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2,,"AT&ZI7=%s<cr>"  

[ISDNOL.JPN]
HKR,ISDN\SwitchType,SWITCH_INS64,,"AT<cr>"   
HKR,ISDN\SetMSN,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2,,"AT&ZI7=%s<cr>"  
HKR,Protocol\ISDN\V110_57DOT6K,1,, "AT&O2B19<cr>"

[OL.Data]
HKR,,Properties,1,00,00,00,00,ff,00,00,00,ff,00,00,00,00,00,00,00,00,00,00,00,31,01,00,00,00,08,07,00,00,f4,01,00
HKR,,DCB, 1,1c,00,00,00,00,c2,01,00,15,20,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FZE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"AT&L1S38.3=1<cr>"
HKR,Init,4,,"ATS84.4=1S118.3=1&K3<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATS118.3=0<cr>"
HKR,Answer, 2,,"ATA<cr>"
HKR,Settings,CallSetupFailTimer,, "S7=<#>"
HKR,Settings,Compression_Off,,"&K00"
HKR,Settings,Compression_On,, "&K44"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,, "P"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"

[OLP.Data]
HKR,, Properties, 1, 00,00,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 07,00,00,00, 33,01,00,00, 00,08,07,00, 00,f4,01,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00,11, 13, 00, 00, 00
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, Reset,, "ATZ<cr>"
;HKR,, UserInit,, "ATB40"
HKR, Init,      1,, "AT&FZE0X8<cr>"
HKR, Init,      2,, "ATV1&D2&C1S0=0<cr>"
HKR, Init,      3,, "AT&L1S38.3=1<cr>"
HKR, Init,      4,, "ATS84.4=1S118.3=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH0<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, Compression_Off,, "&K00"
HKR, Settings, Compression_On,,  "&K44"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, ErrorControl_Off,, "&K0"
HKR, Settings, ErrorControl_On,, "&K3"
HKR, Settings, FlowControl_Hard,,"&H3"
HKR, Settings, FlowControl_Off,, "&H0"
HKR, Settings, FlowControl_Soft,,"&H4"
HKR, Settings, InactivityTimeout,, "S50=<#>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Pulse,, "P"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerVolume_Low,, "L1"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, Tone,, "T"

[ISDNOLP.All]
HKR, EnableCallerID,1,, 					"ats84.4=0<cr>"
HKR, ISDN\Init,1,,                          "AT&O2<cr>"
HKR, ISDN\NvSave,1,,                        "AT<cr>"
HKR, ISDN\NvSave,2,,                        "AT<cr>"

HKR, Protocol\ISDN\AUTO_1CH,1,,             "ATB95&J0S80.6=0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_56K,1,,         "ATB40&J0&E1<cr>"
HKR, Protocol\ISDN\HDLC_PPP_64K,1,,         "ATB40&J0&E0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_112K,1,,        "ATB40&J3&E1<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K,1,,        "ATB40&J3&E0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K_PAP,1,,    "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,   "ATB40&J3&E0S87.2=0S118.3=0<cr>"
;HKR, Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"

HKR, Protocol\ISDN\V120_56K,1,,             "ATB20&J0&E1<cr>"
HKR, Protocol\ISDN\V120_64K,1,,             "ATB20&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\V120_112,1,,             "ATB20&J3&E1<cr>"
HKR, Protocol\ISDN\V120_128K,1,,            "ATB20&J3&E0S80.6=1<cr>"

HKR, Protocol\ISDN\X75_64K,1,,              "ATB00&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\X75_128K,1,,             "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR, Protocol\ISDN\X75_T_70,1,,             "ATB01&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\X75_BTX,1,,              "ATB04&J0&E0S80.6=1<cr>"

HKR, Protocol\ISDN\V110_2DOT4K,1,,          "ATB13S80.6=1<cr>"
HKR, Protocol\ISDN\V110_4DOT8K,1,,          "ATB14S80.6=1<cr>"
HKR, Protocol\ISDN\V110_9DOT6K,1,,          "ATB15S80.6=1<cr>"
HKR, Protocol\ISDN\V110_14DOT4K,1,,         "ATB16S80.6=1<cr>"
HKR, Protocol\ISDN\V110_19DOT2K,1,,         "ATB17S80.6=1<cr>"
HKR, Protocol\ISDN\V110_38DOT4K,1,,         "ATB18<cr>"

[ISDNOP.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\AUTO_1CH,1,, "ATB95&J0S80.6=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"ATB40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"ATB40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "ATB40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "ATB40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"ATB40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"
HKR,Protocol\ISDN\V120_56K ,1,,"ATB20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "ATB20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "ATB20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"ATB20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"ATB00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "ATB01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"ATB04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_2DOT4K,1,, "ATB13S80.6=1<cr>"
HKR,Protocol\ISDN\V110_4DOT8K,1,, "ATB14S80.6=1<cr>"
HKR,Protocol\ISDN\V110_9DOT6K,1,, "ATB15S80.6=1<cr>"
HKR,Protocol\ISDN\V110_14DOT4K,1,,"ATB16S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"ATB17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,, "ATB18<cr>"

[ISDNON.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"ATB40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"ATB40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "ATB40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "ATB40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"ATB40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"
HKR,Protocol\ISDN\V120_56K ,1,,"ATB20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "ATB20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "ATB20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"ATB20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"ATB00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "ATB01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"ATB04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_2DOT4K,1,, "ATB13S80.6=1<cr>"
HKR,Protocol\ISDN\V110_4DOT8K,1,, "ATB14S80.6=1<cr>"
HKR,Protocol\ISDN\V110_9DOT6K,1,, "ATB15S80.6=1<cr>"
HKR,Protocol\ISDN\V110_14DOT4K,1,,"ATB16S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"ATB17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,, "ATB18<cr>"

[ISDNOP.USA]
HKR,ISDN\SwitchType,SWITCH_DMS100,,"ATP0<cr>"   
HKR,ISDN\SwitchType,SWITCH_NI1,,"ATP2<cr>"   
HKR,ISDN\SwitchType,SWITCH_ATT1,, "ATP6<cr>"   
HKR,ISDN,CompatibilityFlags, 1,00,00,00,01
HKR,ISDN\SetSpid,1,,"ATSPID0=%s<cr>"
HKR,ISDN\SetSpid,2,,"ATSPID1=%s<cr>"
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  
HKR,ISDN\NvSave,2,,"ATZ<cr>"

[ISDNOP.1TR6]
HKR,ISDN\SwitchType,SWITCH_1TR6,, "AT<cr>"
HKR,ISDN\SetEAZ,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetEAZ,2 ,,"AT&ZI7=%s<cr>"  
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s<cr>"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  

[ISDNOP.DSS1]
HKR,ISDN\SwitchType,SWITCH_DSS1,, "AT<cr>"
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  

[ISDNOP.JPN]
HKR,ISDN\SwitchType,SWITCH_INS64,,"AT<cr>"   
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  
HKR,Protocol\ISDN\V110_57DOT6K,1,, "ATB19<cr>"

[OP.Data]
HKR,,Properties,1,00,00,00,00,ff,00,00,00,ff,00,00,00,00,00,00,00,00,00,00,00,31,01,00,00,00,08,07,00,00,f4,01,00
HKR,,DCB, 1,1c,00,00,00,00,c2,01,00,15,20,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FZE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"AT&L1S38.3=1<cr>"
HKR,Init,4,,"ATS84.4=1S118.3=1&K3<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATA<cr>"
HKR,Settings,CallSetupFailTimer,, "S7=<#>"
HKR,Settings,Compression_Off,,"&K00"
HKR,Settings,Compression_On,, "&K44"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,ErrorControl_Off,,"&K0"
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,, "P"
HKR,Settings,SpeakerMode_Dial,,"M1"
HKR,Settings,SpeakerMode_Off,,"M0"
HKR,Settings,SpeakerMode_On,, "M2"
HKR,Settings,SpeakerMode_Setup,,"M3"
HKR,Settings,SpeakerVolume_High,, "L3"
HKR,Settings,SpeakerVolume_Low,,"L1"
HKR,Settings,SpeakerVolume_Med,,"L2"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"

[ISDNHT.All]
HKR,ISDN\Init,1,,"ATE0V1<cr>"
HKR,ISDN\NvSave,1,, "AT<cr>"
HKR,Protocol\ISDN\AUTO_1CH,1,, "ATB95&J0S80.6=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_56K,1,,"ATB40&J0&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_64K,1,,"ATB40&J0&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_112K,1,, "ATB40&J3&E1<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K,1,, "ATB40&J3&E0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_PAP,1,, "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR,Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,"ATB40&J3&E0S87.2=0S118.3=0<cr>"
HKR,Protocol\ISDN\V120_56K ,1,,"ATB20&J0&E1<cr>"
HKR,Protocol\ISDN\V120_64K,1,, "ATB20&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V120_112,1,, "ATB20&J3&E1<cr>"
HKR,Protocol\ISDN\V120_128K,1,,"ATB20&J3&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_64K,1,,"ATB00&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_128K,1,, "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR,Protocol\ISDN\X75_T_70,1,, "ATB01&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\X75_BTX,1,,"ATB04&J0&E0S80.6=1<cr>"
HKR,Protocol\ISDN\V110_19DOT2K,1,,"ATB17S80.6=1<cr>"
HKR,Protocol\ISDN\V110_38DOT4K,1,,"ATB18<cr>"



[ISDNT.USA]
HKR,ISDN\SwitchType,SWITCH_DMS100,,"ATP0<cr>"    
HKR,ISDN\SwitchType,SWITCH_NI1,,"ATP2<cr>"   
HKR,ISDN\SwitchType,SWITCH_ATT1,, "ATP6<cr>"   
HKR,ISDN,CompatibilityFlags, 1,00,00,00,01
HKR,ISDN\SetSpid,1,,"ATSPID0=%s<cr>"
HKR,ISDN\SetSpid,2,,"ATSPID1=%s<cr>"
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  
HKR,ISDN\NvSave,2,,"ATZ<cr>"

[ISDNT.1TR6]
HKR,ISDN\SwitchType,SWITCH_1TR6,, "AT<cr>"
HKR,ISDN\SetEAZ,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetEAZ,2 ,,"AT&ZI7=%s<cr>"  
HKR,ISDN\DirectoryNo,1,,"AT&ZI4=%s"  
HKR,ISDN\DirectoryNo,2,,"AT&ZI7=%s<cr>"  

[ISDNT.DSS1]
HKR,ISDN\SwitchType,SWITCH_DSS1,, "AT<cr>"
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  

[ISDNT.JPN]
HKR,ISDN\SwitchType,SWITCH_INS64,,"AT<cr>"   
HKR,ISDN\SetMSN,1 ,,"AT&ZI4=%s<cr>"  
HKR,ISDN\SetMSN,2 ,,"AT&ZI7=%s<cr>"  
HKR,Protocol\ISDN\V110_57DOT6K,1,, "ATB19<cr>"

[ISDN.DSS1]
HKR, ISDN\SwitchType, SWITCH_DSS1,, "AT<cr>"
HKR, ISDN, CompatibilityFlags,             1, 00,00,00,00
HKR, ISDN\SetMSN, 1 ,, "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\SetMSN, 2 ,, "AT&ZI7=%s<cr>"  ; POTS port #1

[ISDN.JAPAN]
HKR, ISDN\SwitchType, SWITCH_INS64,, "AT<cr>"
HKR, ISDN\SwitchType, SWITCH_DSS1,,  "AT<cr>"
HKR, Protocol\ISDN\V110_57DOT6K,1,,  "ATB19<cr>"
HKR, ISDN,CompatibilityFlags,              1, 00,00,00,00
HKR, ISDN\SetMSN,1,, "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\SetMSN,2,, "AT&ZI7=%s<cr>"  ; POTS port #1

[ISDN.USA]
HKR, ISDN\SwitchType, SWITCH_DMS100,, "ATP0<cr>"   ;Northern Telecom DMS-100
HKR, ISDN\SwitchType, SWITCH_NI1,, "ATP1<cr>"   ;National ISDN 1, 1 SPID
HKR, ISDN\SwitchType, SWITCH_NI2,, "ATP2<cr>"   ;National ISDN 1, 2 SPIDs
HKR, ISDN\SwitchType, SWITCH_ATTPTP,, "ATP4<cr>"   ;AT&T 5ESS Custom, Point-to-Point
HKR, ISDN\SwitchType, SWITCH_ATT1,, "ATP5<cr>"   ;AT&T 5ESS Custom, Point-to-MultiPoint, 1 SPID
HKR, ISDN\SwitchType, SWITCH_ATT2,, "ATP6<cr>"   ;AT&T 5ESS Custom, Point-to-MultiPoint, 2 SPIDs

HKR, Responses, "<cr><lf>Switch Type : Northern Telecom DMS<cr><lf>",                   1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI1(1 SPID)<cr><lf>",                            1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI1(2 SPID)<cr><lf>",                            1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI2<cr><lf>",                                    1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI3<cr><lf>",                                    1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-point<cr><lf>",               1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-multipoint(1 SPID)<cr><lf>",  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-multipoint(2 SPID)<cr><lf>",  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "SPID0 =",                                                              1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "SPID1 =",                                                              1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "Please use ATSPIDnn..n to input SPID!<cr><lf>",                        1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "Please Reset TA (Power On/Off) & Reenter SPID(s)",                     1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>WARNING: No Channel(SPID) Available<cr><lf>",                  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>WARNING: Layer 1 Not Active<cr><lf>",                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Don't need SPID in AT&T P-t-P mode!<cr><lf>",                  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID correct!<cr><lf>",                                        1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID Error!<cr><lf>",                                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID correct! Full Service.<cr><lf>",                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID not correct! Restricted Service.<cr><lf>",                1, 00, 00, 00,00,00,00, 00,00,00,00

HKR, ISDN, CompatibilityFlags,             1, 00,00,00,01
HKR, ISDN\SetSpid, 1,,  "ATSPID0=%s<cr>"
HKR, ISDN\SetSpid, 2,,  "ATSPID1=%s<cr>"
HKR, ISDN\DirectoryNo, 1,,  "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\DirectoryNo, 2,,  "AT&ZI7=%s<cr>"  ; POTS port #1

[OT.Data]
HKR,,Properties,1,00,00,00,00,ff,00,00,00,ff,00,00,00,00,00,00,00,00,00,00,00,31,01,00,00,00,08,07,00,00,f4,01,00
HKR,,DCB, 1,1c,00,00,00,00,c2,01,00,15,20,00,00,00,00,0a,00,0a,00,08,00,00,11,13,00,00,00
HKR,,InactivityScale,1,0a,00,00,00
HKR,,Reset,,"ATZ<cr>"
HKR,Init,1,,"AT&FZE0X7<cr>"
HKR,Init,2,,"ATV1&D2&C1S0=0<cr>"
HKR,Init,3,,"AT&L1S38.3=1<cr>"
HKR,Init,4,,"ATS84.4=1S118.3=1<cr>"
HKR,Monitor,1,,"ATS0=0<cr>"
HKR,Monitor,2,,"None"
HKR,Hangup, 1,,"ATH0<cr>"
HKR,Answer, 1,,"ATA<cr>"
HKR,Settings,CallSetupFailTimer,, "S7=<#>"
HKR,Settings,ErrorControl_Off,,"&K0"
HKR,Settings,Compression_Off,,"&K00"
HKR,Settings,Compression_On,, "&K44"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,FlowControl_Hard,,"&H3"
HKR,Settings,FlowControl_Off,,"&H0"
HKR,Settings,FlowControl_Soft,,"&H4"
HKR,Settings,InactivityTimeout,,"S50=<#>"
HKR,Settings,Prefix,,"AT"
HKR,Settings,Pulse,, "P"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,Tone,,"T"

[Fax2DRAM]
HKR, Monitor, 1,,        "ATZ<cr>"

[E2864V90.Fax]
HKR, Fax\Class1\AdaptiveAnswer,SetupCommand,,   "ATS38.3=0"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 1,, "AT+FCLASS=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 2,, "ATS57.7=1+FAE=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 3,, "ATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxDetect,, "FAX"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxConnect,, "CONNECT"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataDetect,,"DATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataConnect,,  "CONNECT"

[OM90.Fax]
HKR, Fax\Class1\AdaptiveAnswer,SetupCommand,,              "AT"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 1,,          "AT+FCLASS=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              2,, "ATS57.7=1+FAE=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              3,, "ATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxDetect,,    "FAX"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxConnect,,   "CONNECT"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataDetect,,   "DATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataConnect,,  "CONNECT"

[OLM.Fax]
HKR, Fax\Class1\AdaptiveAnswer,SetupCommand,,              "AT&D3&K4"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              1,, "AT+FCLASS=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              2,, "AT+FAE=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              3,, "ATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxDetect,,    "FAX"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxConnect,,   "CONNECT"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataDetect,,   "DATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataConnect,,  "CONNECT"
HKR, Fax, ExitCommand,,                                     "ATZ"
HKR, Fax, FixSerialSpeed,,                                 "14400"
HKR, Fax, HighestSendSpeed,,                               "14400"
HKR, Fax, LowestSendSpeed,,                                "2400"

[E2864.voice]
HKR,,Enumerator,,serwave.vxd
HKR,, VoiceProfile,    			1,23,30,01,02
HKR, WaveDriver,  BaudRate,         1, 00,c2,01,00
HKR, WaveDriver,  XformID,          1, 0b,00
HKR, WaveDriver,  WaveDevices,      1, 02,00
HKR, WaveDriver,  XformModule,    , "umdmxfrm.dll"
HKR, WaveDriver,  WaveHardwareID, , "HALFDUPLEX"
HKR,, HandsetCloseDelay,           1, 1e,00,00,00
HKR, HandsetSetRecordFormat,       1,,"at+vsm=80,8000<cr>"
HKR, HandsetSetRecordFormat,       2,,"at+vls=8<cr>"
HKR, HandsetSetPlayFormat,         1,,"at+vsm=80,8000<cr>"
HKR, HandsetSetPlayFormat,         2,,"at+vls=16<cr>"
HKR, LineSetRecordFormat,          1,,"at+vsm=80,8000<cr>"
HKR, LineSetRecordFormat,          2,,"at+vls=2<cr>"
HKR, LineSetPlayFormat,            1,,"at+vsm=80,8000<cr>"
HKR, LineSetPlayFormat,            2,,"at+vls=2<cr>"
HKR, OpenHandset,                  1,, "at+fclass=8<cr>"
HKR, OpenHandset,                  2,, "at+vls=1<cr>"
HKR, CloseHandset,                 1,, "at+vls=0<cr>"
HKR, CloseHandset,                 2,, "at+fclass=0<cr>"
HKR, StartPlay,                    1,, "at+vtx<cr>"
HKR, StopPlay,                     1,, "None"
HKR, StopPlay,                     2,, "NoResponse"
HKR, StartRecord,                  1,, "at+vrx<cr>"
HKR, StopRecord,                   1,, "None"
HKR, StopRecord,                   2,, "NoResponse"
HKR,, TerminateRecord,,            "!"
HKR,, TerminatePlay,,              "<h10><h03>"
HKR,, AbortPlay,,                  "<h10><h18>"
HKR, VoiceToDataAnswer,            1,, "at+fclass=0<cr>"
HKR, VoiceToDataAnswer,            2,, "ata<cr>"
HKR, VoiceAnswer,                  1,, "at+fclass=8<cr>"
HKR, VoiceAnswer,                  2,, "at+vit=0<cr>"
HKR, VoiceAnswer,                  3,, "at+flo=1<cr>"
HKR, VoiceAnswer,                  4,, "at+vsm=80,8000<cr>"
HKR, VoiceAnswer,                  5,, "at+vls=2<cr>"
HKR, VoiceAnswer,                  6,, "ata<cr>"
HKR, VoiceDialNumberSetup,         1,, "at+fclass=8<cr>"
HKR, VoiceDialNumberSetup,         2,, "at+vtd=50,70<cr>"
HKR, VoiceDialNumberSetup,         3,, "at+vrn=0<cr>"
HKR, VoiceDialNumberSetup,         4,, "at+vsm=80,8000<cr>"
HKR,, CallerIDPrivate,,            P
HKR,, CallerIDOutSide,,            O
HKR,, VariableTerminator,,         <cr><lf>
HKR,, ForwardDelay,                1,88,13
HKR, GenerateDigit,                1,, "at+vts=<Digit><cr>"
HKR, EnableCallerID,               1,, "ats40.2=1<cr>"
HKR, Responses, "<cr><lf>VCON<cr><lf>",                  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATE=",                         1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>TIME: ",                        1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CALLER NUMBER: ",               1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>REASON FOR NO CALLER NUMBER: ", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CALLER NAME: ",                 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>REASON FOR NO CALLER NAME: ",   1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 1<cr><lf>",                1, 19, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 2<cr><lf>",                1, 1a, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 3<cr><lf>",                1, 1a, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 4<cr><lf>",                1, 1a, 00, 00,00,00,00, 00,00,00,00

[OM90.voice]
HKR,,Enumerator,,serwave.vxd
HKR,,VoiceProfile,                      1,23,30,01,02
HKR,,HandsetCloseDelay,                 1,01,00,00,00
HKR, WaveDriver,  BaudRate,             1, 00,c2,01,00 
HKR, WaveDriver, XformModule,  , "umdmxfrm.dll"
HKR,WaveDriver,XformID, 1, 04,00
HKR,WaveDriver,WaveDevices,  1, 02, 00
HKR, WaveDriver,  WaveHardwareID, , "HALFDUPLEX"

; voice sampling format is 4-bit ADPCM at 8000 Hz
HKR, HandsetSetRecordFormat,        1,,"at+vsm=4,8000<cr>"
HKR, HandsetSetPlayFormat,          1,,"at+vsm=4,8000<cr>"
HKR, LineSetRecordFormat,           1,,"at+vsm=4,8000<cr>"
HKR, LineSetPlayFormat,             1,,"at+vsm=4,8000<cr>"

HKR, OpenHandset,                   1,, "at+fclass=8<cr>"
HKR, OpenHandset,                   2,, "at+vls=1<cr>"
HKR, CloseHandset,                  1,, "ath<cr>"

HKR, StartPlay,                     1,, "at+vtx<cr>"
HKR, StopPlay,                      1,, "None"
HKR, StopPlay,                      2,, "NoResponse"

HKR, StartRecord,                   1,, "at+vrx<cr>"
HKR, StopRecord,                    1,, "None"
HKR, StopRecord,                    2,, "NoResponse"

HKR,, TerminateRecord,,             "!"
HKR,, TerminatePlay,,               "<h10><h03>"
HKR,, AbortPlay,,                   "<h10><h18>"

HKR, VoiceToDataAnswer,             1,,"at+fclass=0<cr>"
HKR, VoiceToDataAnswer,             2,,"ata<cr>"

HKR, VoiceAnswer,                   1,, "at+fclass=8<cr>"
HKR, VoiceAnswer,                   2,, "at+vit=0<cr>"
HKR, VoiceAnswer,                   3,, "at+flo=1<cr>"
HKR, VoiceAnswer,                   4,, "at+vsm=4,8000<cr>"
HKR, VoiceAnswer,                   5,, "ata<cr>"

HKR, VoiceDialNumberSetup,          1,, "at+fclass=8<cr>"
HKR, VoiceDialNumberSetup,          2,, "at+vrn=0<cr>"
HKR, VoiceDialNumberSetup,          3,, "at+vsm=4,8000<cr>"

HKR,, CallerIDPrivate,,             PRIVACY
HKR,, CallerIDOutSide,,             OUT-OF-AREA
HKR,, VariableTerminator,,          <cr><lf>
HKR,, ForwardDelay,                 1,88,13

HKR, GenerateDigit,                 1,, "at+vts=<Digit><cr>"
HKR, EnableCallerID,                1,, "ats40.2=1<cr>"

HKR, EnableDistinctiveRing,         1,, "ats40.6=1<cr>"
HKR, EnableDistinctiveRing,         2,, "ats40.5=1<cr>"
HKR, EnableDistinctiveRing,         3,, "ats40.4=1<cr>"
HKR, EnableDistinctiveRing,         4,, "ats40.3=1<cr>"

HKR, Responses, "<cr><lf>VCON<cr><lf>",                     1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATE=",                            1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>TIME: ",                           1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CALLER NUMBER: ",                  1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>REASON FOR NO CALLER NUMBER: ",    1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CALLER NAME: ",                    1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>REASON FOR NO CALLER NAME: ",      1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 1<cr><lf>",                   1, 19, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 2<cr><lf>",                   1, 1a, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 3<cr><lf>",                   1, 1a, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING 4<cr><lf>",                   1, 1a, 00, 00,00,00,00, 00,00,00,00


[Additional.Responses]
; extended CARRIER (ISDN) responses
HKR, Responses, "<cr><lf>CARRIER 38400<cr><lf>",           1, 01, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 57600<cr><lf>",           1, 01, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 64000<cr><lf>",           1, 01, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 112K<cr><lf>",            1, 01, 00, 80,B5,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 128K<cr><lf>",            1, 01, 00, 00,F4,01,00, 00,00,00,00
; B-channel protocol (ISDN)
HKR, Responses, "<cr><lf>PROTOCOL: V110<cr><lf>",           1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: PPP<cr><lf>",            1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: SLIP<cr><lf>",           1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75<cr><lf>",           1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75M<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75C<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120<cr><lf>",           1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120M<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120C<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: BTX<cr><lf>",            1, 01, 00, 00,00,00,00, 00,00,00,00
; Error control protocol (ISDN)
HKR, Responses, "<cr><lf>ERROR CONTROL: NONE<cr><lf>",                 1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPB<cr><lf>",                 1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPD<cr><lf>",                 1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: ARQ<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00

[OM90.Responses]
; standard CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 300<cr><lf>",             1, 01, 00, 2c,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 1200<cr><lf>",            1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 2400<cr><lf>",            1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 4800<cr><lf>",            1, 01, 00, c0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 7200<cr><lf>",            1, 01, 00, 20,1c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 9600<cr><lf>",            1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 12000<cr><lf>",           1, 01, 00, e0,2e,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 14400<cr><lf>",           1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 16800<cr><lf>",           1, 01, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 19200<cr><lf>",           1, 01, 00, 00,4b,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38400<cr><lf>", 		1, 01, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 21600<cr><lf>",           1, 01, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 24000<cr><lf>",           1, 01, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 26400<cr><lf>",           1, 01, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 28800<cr><lf>",           1, 01, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 31200<cr><lf>",           1, 01, 00, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33600<cr><lf>",           1, 01, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 75/1200<cr><lf>",         1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 1200/75<cr><lf>",         1, 01, 00, b0,04,00,00, 00,00,00,00

; extended CARRIER (V.90) responses
HKR, Responses, "<cr><lf>CARRIER 28000<cr><lf>",           1, 01, 00, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 29333<cr><lf>",           1, 01, 00, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 30666<cr><lf>",           1, 01, 00, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 32000<cr><lf>",           1, 01, 00, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33333<cr><lf>",           1, 01, 00, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 34666<cr><lf>",           1, 01, 00, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 36000<cr><lf>",           1, 01, 00, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 37333<cr><lf>",           1, 01, 00, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38666<cr><lf>",           1, 01, 00, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 40000<cr><lf>",           1, 01, 00, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 41333<cr><lf>",           1, 01, 00, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 42666<cr><lf>",           1, 01, 00, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 44000<cr><lf>",           1, 01, 00, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 45333<cr><lf>",           1, 01, 00, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 46666<cr><lf>",           1, 01, 00, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 48000<cr><lf>",           1, 01, 00, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 49333<cr><lf>",           1, 01, 00, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 50666<cr><lf>",           1, 01, 00, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 52000<cr><lf>",           1, 01, 00, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 53333<cr><lf>",           1, 01, 00, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 54666<cr><lf>",           1, 01, 00, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 56000<cr><lf>",           1, 01, 00, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 57600<cr><lf>", 		1, 01, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 64000<cr><lf>", 		1, 01, 00, 00,FA,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>COMPRESSION: None<cr><lf>",            1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: MNP5<cr><lf>",            1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: V42b<cr><lf>",            1, 01, 01, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>PROTOCOL: None<cr><lf>",               1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: MNP4<cr><lf>",               1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V42<cr><lf>",                1, 01, 02, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",            1, 02, 00, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",            1, 02, 00, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",            1, 02, 00, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",            1, 02, 00, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",           1, 02, 00, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",           1, 02, 00, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",           1, 02, 00, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",          1, 02, 00, 00,00,00,00, 00,c2,01,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",          1, 02, 00, 00,00,00,00, 00,84,03,00
HKR, Responses, "<cr><lf>CONNECT 460800<cr><lf>",          1, 02, 00, 00,00,00,00, 00,08,07,00

[OL.Responses]
HKR, Responses, "<cr><lf>CARRIER 2400<cr><lf>", 		1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 4800<cr><lf>", 		1, 01, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 9600<cr><lf>", 		1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 14400<cr><lf>", 		1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 19200<cr><lf>", 		1, 01, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38400<cr><lf>", 		1, 01, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 57600<cr><lf>", 		1, 01, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 56000<cr><lf>", 		1, 01, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 64000<cr><lf>", 		1, 01, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 112K<cr><lf>", 		1, 01, 00, 80,B5,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 128K<cr><lf>", 		1, 01, 00, 00,F4,01,00, 00,00,00,00

HKR, Responses, "<cr><lf>PROTOCOL: V110<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: PPP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: SLIP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: BTX<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>ERROR CONTROL: NONE<cr><lf>", 	1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPB<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPD<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>COMPRESSION: V42b<cr><lf>", 	1, 01, 01, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",        	1, 02, 00, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",        	1, 02, 00, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",         1, 02, 00, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",         1, 02, 00, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",        1, 02, 00, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",        1, 02, 00, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",        1, 02, 00, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",       1, 02, 00, 00,00,00,00, 00,c2,01,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",       1, 02, 00, 00,00,00,00, 00,84,03,00
HKR, Responses, "<cr><lf>CONNECT 460800<cr><lf>",       1, 02, 00, 00,00,00,00, 00,08,07,00
HKR, Responses, "<cr><lf>CONNECT    USB<cr><lf>",       1, 02, 00, 00,00,00,00, 00,c2,01,00
;HKR, Responses, "<cr><lf>CONNECT    USB<cr><lf>",       1, 02, 00, 00,00,00,00, 00,00,00,00

[OLM.Responses]
; ISDN CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 2400<cr><lf>", 		1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 4800<cr><lf>", 		1, 01, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 9600<cr><lf>", 		1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 14400<cr><lf>", 		1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 19200<cr><lf>", 		1, 01, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38400<cr><lf>", 		1, 01, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 57600<cr><lf>", 		1, 01, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 56000<cr><lf>", 		1, 01, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 64000<cr><lf>", 		1, 01, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 112K<cr><lf>", 		1, 01, 00, 80,B5,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 128K<cr><lf>", 		1, 01, 00, 00,F4,01,00, 00,00,00,00

; extended modem CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 1200<cr><lf>", 		1,  01,  00,  B0,04,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 7200<cr><lf>", 		1,  01,  00,  20,1C,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 12000<cr><lf>", 		1,  01,  00,  E0,2E,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 16800<cr><lf>",                1,  01,  00,  A0,41,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 21600<cr><lf>", 		1,  01,  00,  60,54,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 24000<cr><lf>", 		1,  01,  00,  C0,5D,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 26400<cr><lf>", 		1,  01,  00,  20,67,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 28800<cr><lf>", 		1,  01,  00,  80,70,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 31200<cr><lf>", 		1,  01,  00,  E0,79,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33600<cr><lf>", 		1,  01,  00,  40,83,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 28000<cr><lf>", 		1,  01,  00,  60,6D,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 29333<cr><lf>", 		1,  01,  00,  95,72,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 30666<cr><lf>", 		1,  01,  00,  CA,77,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 32000<cr><lf>", 		1,  01,  00,  00,7D,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33333<cr><lf>", 		1,  01,  00,  35,82,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 34000<cr><lf>", 		1,  01,  00,  D0,84,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 34666<cr><lf>", 		1,  01,  00,  6A,87,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 36000<cr><lf>", 		1,  01,  00,  A0,8C,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 37333<cr><lf>", 		1,  01,  00,  D5,91,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38000<cr><lf>", 		1,  01,  00,  70,94,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38666<cr><lf>", 		1,  01,  00,  0A,97,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 40000<cr><lf>", 		1,  01,  00,  40,9C,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 41333<cr><lf>", 		1,  01,  00,  75,A1,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 42000<cr><lf>", 		1,  01,  00,  10,A4,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 42666<cr><lf>", 		1,  01,  00,  AA,A6,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 44000<cr><lf>", 		1,  01,  00,  E0,AB,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 45333<cr><lf>", 		1,  01,  00,  15,B1,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 46666<cr><lf>", 		1,  01,  00,  4A,B6,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 48000<cr><lf>", 		1,  01,  00,  80,BB,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 49333<cr><lf>", 		1,  01,  00,  B5,C0,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 50000<cr><lf>", 		1,  01,  00,  50,C3,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 50666<cr><lf>", 		1,  01,  00,  EA,C5,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 52000<cr><lf>", 		1,  01,  00,  20,CB,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 53333<cr><lf>", 		1,  01,  00,  55,D0,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 54000<cr><lf>", 		1,  01,  00,  F0,D2,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 54666<cr><lf>", 		1,  01,  00,  8A,D5,00,00,  00,00,00,00

; ISDN B-channel protocol 
HKR, Responses, "<cr><lf>PROTOCOL: V110<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: PPP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: SLIP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: BTX<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00

; Modem protocol
HKR, Responses, "<cr><lf>PROTOCOL: NONE<cr><lf>", 			1,  01,  00,  00,00,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: LAPM<cr><lf>", 			1,  01,  00,  00,00,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: ALT<cr><lf>", 			1,  01,  00,  00,00,00,00,  00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: ALT-CELLULAR<cr><lf>", 	1,  01,  00,  00,00,00,00,  00,00,00,00

; ISDN & Modem error control protocol
HKR, Responses, "<cr><lf>ERROR CONTROL: NONE<cr><lf>", 	1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPB<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPD<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: ARQ<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00

; ISDN & Modem compression protocol
HKR, Responses, "<cr><lf>COMPRESSION: MNP5<cr><lf>",       	1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: V42b<cr><lf>",       	1, 01, 01, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",        	1, 02, 00, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",        	1, 02, 00, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",         1, 02, 00, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",         1, 02, 00, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",        1, 02, 00, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",        1, 02, 00, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",        1, 02, 00, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",       1, 02, 00, 00,00,00,00, 00,c2,01,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",       1, 02, 00, 00,00,00,00, 00,84,03,00
HKR, Responses, "<cr><lf>CONNECT 460800<cr><lf>",       1, 02, 00, 00,00,00,00, 00,08,07,00


[ZD56.NT.Services]
AddService=usbser, 0x00000000, LowerFilter_Service_Inst

[ZD56.NT.HW]
AddReg=LowerFilterAddReg

[LowerFilterAddReg]
HKR,,"LowerFilters",0x00010000,"usbser"

[LowerFilter_Service_Inst]
DisplayName=%USBFilterString%
ServiceType= 1
StartType  = 3
ErrorControl = 0
ServiceBinary = %12%\usbser.sys

[FakeModemCopyFileSection]
usbser.sys,,,0x20

[DestinationDirs]
FakeModemCopyFileSection=12
DefaultDestDir = 12
