; UNIMODEM5 ISDN INF MDMBUG.inf
; Copyright 2000 Microsoft Co.,Ltd.
; Copyright 2000 B.U.G.
;

[Version]
LayoutFile=Layout.inf
Provider=%MSFT%
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
DriverVer=07/01/2001,5.1.2535.0

[Manufacturer]
%Mfg% = Models


; Modem models

[ControlFlags]
ExcludeFromSelect=*

[Models]
%ISDN1% = ISDN1,PCMCIA\B.U.G._INC.-LINKBOY_D128-CDCB		;BUG Linkboy D128


; Installation sections

[ISDN1]
AddReg=All_ISDN,MfgAddAll_ISDN,PCMCIA,ISDN1.AddReg

[ISDN1.AddReg]  ;BUG Linkboy D128
HKR,, Properties, 1, 00,00,00,00, 32,00,00,00, ff,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,c2,01,00, 00,f4,01,00

[Strings]
MSFT="Microsoft"
Mfg = "B.U.G."
ISDN1 = "BUG Linkboy D128"


[All_ISDN]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,      1,, "AT<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>", 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>", 1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>", 1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>", 1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>", 1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED<cr><lf>", 1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "0<cr>",  		1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>",  		1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT
HKR, Responses, "2<cr>",  		1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>",  		1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",  		1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "5<cr>",  		1, 02, 00, B0,04,00,00, 00,00,00,00 ; CONNECT 1200
HKR, Responses, "6<cr>",  		1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",  		1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",  		1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

[PCMCIA]
HKR,,PortDriver,,Serial.vxd
HKR,,Contention,,*vcd
HKR,,DeviceType, 1, 03
HKR,,PowerDelay,1, DC,05,00,00

[MfgAddAll_ISDN]
HKR, Settings,  CallSetupFailTimer,,"S7=<#>"
HKR, Settings, InactivityTimeout,,"\T<#>"
HKR,, InactivityScale, 1, 0a,00,00,00
HKR, Init, 2,,"AT&FE0X1<cr>"
HKR, Init, 3,,"ATQ0V1&C1&D2&E0&S0!A0S0=0<cr>"
HKR, Monitor, 1,,"ATS0=0<cr>"
HKR, Monitor, 2,,"None"
HKR, Hangup, 1,,"ATH<cr>"
HKR, Answer, 1,,"ATA<cr>"
HKR,, Reset,,"ATZ<cr>"
HKR, Settings,  Prefix,,"AT"
HKR, Settings,  Terminator,,"<cr>"
HKR, Settings,  DialPrefix,,"D"
HKR, Settings,  DialSuffix,, ""
HKR, Settings,  FlowControl_Off,,"\Q0"
HKR, Settings,  FlowControl_Hard,,"\Q3"
HKR, Settings,  FlowControl_Soft,,"\Q1"
HKR, Responses,"<cr><lf>CONNECT 9600<cr><lf>", 1,02,00, 80,25,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 19200<cr><lf>", 1,02,00, 00,4b,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 32000<cr><lf>", 1,02,00, 00,7d,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 38400<cr><lf>", 1,02,00, 00,96,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 56000<cr><lf>", 1,02,00, c0,da,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 64000<cr><lf>", 1,02,00, 00,fa,00,00, 00,00,00,00
HKR, Responses,"<cr><lf>CONNECT 128000<cr><lf>", 1,02,00, 00,f4,01,00, 00,00,00,00
HKR, Protocol\ISDN\HDLC_PPP_56K,1,,"AT&Q5$S10S146=1S172=0%%B10<cr>"
HKR, Protocol\ISDN\HDLC_PPP_64K,1,,"AT&Q5$S12S146=1S172=0%%B12<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K,1,,"AT&Q5$S12S146=1S172=1S0=3!G51%%B14<cr>"
HKR, Protocol\ISDN\V110_9DOT6K,1,,"AT&Q0$S5%%B5<cr>"
HKR, Protocol\ISDN\V110_19DOT2K,1,,"AT&Q0$S7%%B7<cr>"
HKR, Protocol\ISDN\V110_38DOT4K,1,,"AT&Q0$S8%%B8<cr>"
HKR, Protocol\ISDN\AUTO_1CH,1,,"AT&Q7S146=1!C0%%B12<cr>"
HKR, Protocol\ISDN\AUTO_2CH,1,,"AT&Q7S146=1!C0S0=3S172=1!G51%%B14<cr>"
