; Copyright (c) 1993-1999 Microsoft Corporation
[Version]
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
LayoutFile=layout.inf
DriverVer=07/01/2001,5.1.2535.0

[Manufacturer]
%VoiceView% = VoiceView
%Motorola%=Motorola

[ControlFlags]
ExcludeFromSelect=*

[VoiceView]
%VVGen288% = VVGen288, MDMVVGEN288
%PNPC112% = PNPC112, *PNPC112
%PNPC113% = PNPC113, *PNPC113
%PNPC116% = PNPC116, *PNPC116
%PNPC117% = PNPC117, *PNPC117
%PNPC11A% = PNPC11A, *PNPC11A
%PNPC11B% = PNPC11B, *PNPC11B
%PNPC11E% = PNPC11E, *PNPC11E
%PNPC11F% = PNPC11F, *PNPC11F

[Motorola]
%Modem01PNP%=MOT_01, SERENUM\MOT1511

[PNPC112]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, Gen288Reg, EXTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC113]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, GenAnyReg, EXTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[VVGen288]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, Gen288Reg, EXTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC116]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, EnhancedAddReg, Enh288Reg, EXTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC117]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, EnhancedAddReg, EnhAnyReg, EXTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[MOT_01]
DriverVer=03/09/2000
AddReg=All,GenericAddReg,EnhancedAddReg,Moto.AddReg,EXTERNAL,MotoVoice,MotoTerse.Resp

[PNPC11A]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, Gen288Reg, INTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC11B]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, GenAnyReg, INTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC11E]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, EnhancedAddReg, Enh288Reg, INTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[PNPC11F]
DriverVer=03/09/2000
include=MDMGL003.INF
AddReg      = All, GenericAddReg, EnhancedAddReg, EnhAnyReg, INTERNAL, MDMGL003.VERBOSE, MDMGL003.VERBOSE2, MDMGL003.VERBOSE3

[Gen288Reg]
HKR,, Properties, 1, 80,01,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,01,00,00, 00,c2,01,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,96,00,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[GenAnyReg]
HKR,, Properties, 1, 80,01,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,01,00,00, 00,c2,01,00, 00,c2,01,00
HKR,, DCB, 1, 1C,00,00,00, 80,25,00,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[Enh288Reg]
HKR,, Properties, 1, 80,01,00,00, 00,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, 00,03,00,00, 00,c2,01,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,96,00,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[EnhAnyReg]
HKR,, Properties, 1, 80,01,00,00, 00,00,00,00, 00,00,00,00, 07,00,00,00, 0f,00,00,00, 00,03,00,00, 00,c2,01,00, 00,c2,01,00
HKR,, DCB, 1, 1C,00,00,00, 80,25,00,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[Moto.AddReg]
HKR,, Properties, 1, 80,01,00,00, FF,00,00,00, FF,00,00,00, 07,00,00,00, 0F,00,00,00, 77,03,00,00, 00,C2,01,00, C0,DA,00,00
HKR,,InactivityScale, 1, 0a,00,00,00
HKR, Init,      2,, "AT&FE0V1&C1&D2W2\V0S0=0<cr>"  ; terse response init
HKR, Settings, Compression_Off,, "%%C"
HKR, Settings, Compression_On,, "%%C3"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, ErrorControl_Off,, "\N"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, ErrorControl_Forced,, "\N2"
HKR, Settings, FlowControl_Off,, "&K"
HKR, Settings, FlowControl_Hard,, "&K3"
HKR, Settings, FlowControl_Soft,, "&K4"
HKR, Settings, InactivityTimeout,, "S30=<#>"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, Modulation_CCITT,, "B"
HKR, Settings, Modulation_Bell,, "B1"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Pulse,, "P"
HKR, Settings, SpeakerVolume_Low,, "L1"

[Strings]
MSFT ="Microsoft"

VoiceView = "Voiceview Compatible Data-Fax"
VVGen288 = "标准 28800 bps 调制解调器"
PNPC112 = "标准 28800 bps 调制解调器"
PNPC113 = "标准调制解调器"
PNPC116 = "标准 28800 bps 调制解调器"
PNPC117 = "标准调制解调器"
PNPC11A = "标准 28800 bps 调制解调器"
PNPC11B = "标准调制解调器"
PNPC11E = "标准 28800 bps 调制解调器"
PNPC11F = "标准调制解调器"
StartXfer_DESC   = "标准自动检测"   ; Name for auto start feature

Motorola="Motorola"
Modem01PNP="Motorola 56K Data Fax Voice PnP MC143450RDK"

[All]
HKR,,FriendlyDriver,,Unimodem.vxd
HKR,,DevLoader,,*VCOMM
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"

[GenericAddReg]
HKR, Init, 1,, "AT<cr>"
HKR, Init, 2,, "ATE0V1<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Answer, 1,, "ATA<cr>"
HKR, Hangup, 1,, "ATH<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, DialSuffix,, ""

[EXTERNAL]
HKR,, DeviceType, 1, 01

[EnhancedAddReg]
HKR, Settings, DialSuffix,, ";"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, SpeakerVolume_Low,, "L0"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"

[INTERNAL]
HKR,, DeviceType, 1, 02

[MotoTerse.Resp]
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "0<cr>",  1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed
HKR, Responses, "1<cr>",  1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT - Connection
HKR, Responses, "2<cr>",  1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING - Ring signal indicated
HKR, Responses, "3<cr>",  1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",  1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command
HKR, Responses, "5<cr>",  1, 02, 00, B0,04,00,00, 00,00,00,00 ; CONNECT 1200
HKR, Responses, "6<cr>",  1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE - No dial tone detected
HKR, Responses, "7<cr>",  1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY - Engaged (busy) signal
HKR, Responses, "8<cr>",  1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
HKR, Responses, "9<cr>",  1, 02, 00, 58,02,00,00, 00,00,00,00 ; CONNECT 600
HKR, Responses, "<cr><lf>CONNECT 600<cr><lf>", 1, 02, 00, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>", 1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>", 1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>", 1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>", 1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200<cr><lf>", 1, 02, 00, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000<cr><lf>", 1, 02, 00, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>", 1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800<cr><lf>", 1, 02, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>", 1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600<cr><lf>", 1, 02, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000<cr><lf>", 1, 02, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400<cr><lf>", 1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>", 1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200<cr><lf>", 1, 02, 00, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000<cr><lf>", 1, 02, 00, 00,7D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>", 1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000<cr><lf>", 1, 02, 00, D0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000<cr><lf>", 1, 02, 00, A0,8C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000<cr><lf>", 1, 02, 00, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>", 1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000<cr><lf>", 1, 02, 00, 40,9C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000<cr><lf>", 1, 02, 00, 10,A4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000<cr><lf>", 1, 02, 00, E0,AB,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000<cr><lf>", 1, 02, 00, B0,B3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000<cr><lf>", 1, 02, 00, 80,BB,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000<cr><lf>", 1, 02, 00, 50,C3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000<cr><lf>", 1, 02, 00, 20,CB,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000<cr><lf>", 1, 02, 00, F0,D2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000<cr><lf>", 1, 02, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>", 1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000<cr><lf>", 1, 02, 00, 90,E2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000<cr><lf>", 1, 02, 00, 60,EA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",1, 02, 00, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",1, 02, 00, 00,84,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000<cr><lf>", 1, 02, 00, 60,6D,8C,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333<cr><lf>", 1, 02, 00, 95,72,8C,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666<cr><lf>", 1, 02, 00, CA,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333<cr><lf>", 1, 02, 00, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666<cr><lf>", 1, 02, 00, 6A,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333<cr><lf>", 1, 02, 00, D5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666<cr><lf>", 1, 02, 00, 0A,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333<cr><lf>", 1, 02, 00, 75,A1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666<cr><lf>", 1, 02, 00, AA,A6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333<cr><lf>", 1, 02, 00, 15,B1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666<cr><lf>", 1, 02, 00, 4A,B6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333<cr><lf>", 1, 02, 00, B5,C0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666<cr><lf>", 1, 02, 00, EA,C5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333<cr><lf>", 1, 02, 00, 55,D0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666<cr><lf>", 1, 02, 00, 8A,D5,00,00, 00,00,00,00

[MotoVoice]
HKR,, Enumerator,,serwave.vxd
HKR,, VoiceProfile,1,25,60,19,02
HKR,WaveDriver, XformModule,  , "umdmxfrm.dll"
HKR,WaveDriver, XformID,     1, 03, 00
HKR,WaveDriver, WaveDevices, 1, 01, 00
HKR,WaveDriver,	BaudRate,    1, 00, c2, 01, 00
HKR,WaveDriver,	WaveHardwareID ,, "MotorolaMC143450RDKWaveDevice"
HKR,, VoiceBaudRate,    1, 00,c2,01,00
HKR, EnableCallerID, 1,, "at#cid=1<cr>"
HKR,, HandsetCloseDelay,     1,1e,00,00,00
HKR, StartPlay,               1,, "at#vtx<cr>"
HKR, StopPlay,                1,, "at<cr>"
HKR, StartRecord,             1,, "at#vrx<cr>"
HKR, StopRecord,              1,, "at<cr>"
HKR,, TerminatePlay,,        "<h10><h03>"
HKR,, TerminateRecord,,      "<cr>"
HKR,, AbortPlay,,            "<h10><h18>"
HKR, LineSetPlayFormat,       1,, "at#vls=0<cr>"
HKR, LineSetRecordFormat,     1,, "None"
HKR, LineSetRecordFormat,     2,, "NoResponse"
HKR, HandsetSetRecordFormat,   1,,"at#vsr=7200<cr>"
HKR, HandsetSetRecordFormat,   2,,"at#vbs=4<cr>"
HKR, HandsetSetPlayFormat,     1,,"at#vsr=7200<cr>"
HKR, HandsetSetPlayFormat,     2,,"at#vbs=4<cr>"
HKR, OpenHandset,               1,, "at#cls=8<cr>"
HKR, OpenHandset,               2,, "at#vls=1<cr>"
HKR, CloseHandset,                   1,, "at#vls=0<cr>"
HKR, CloseHandset,                   2,, "at#cls=0<cr>"
HKR, VoiceToDataAnswer,          1,,"at#cls=0<cr>"
HKR, VoiceToDataAnswer,          2,,"ata<cr>"
HKR, VoiceAnswer,               1,, "at#cls=8<cr>"
HKR, VoiceAnswer,               2,, "at#vls=0<cr>"
HKR, VoiceAnswer,               3,, "at#vbt=1<cr>"
HKR, VoiceAnswer,               4,, "at#vsr=7200<cr>"
HKR, VoiceAnswer,               5,, "at#vbs=4<cr>"
HKR, VoiceAnswer,               6,, "ats30=60<cr>"
HKR, VoiceAnswer,               7,, "ata<cr>"
HKR, VoiceDialNumberSetup,      1,, "at#cls=8<cr>"
HKR, VoiceDialNumberSetup,      2,, "at#vls=0<cr>"
HKR, VoiceDialNumberSetup,      3,, "at#vrn=0<cr>"
HKR, VoiceDialNumberSetup,      4,, "at#vbt=1<cr>"
HKR, VoiceDialNumberSetup,      5,, "at#vsr=7200<cr>"
HKR, VoiceDialNumberSetup,      6,, "at#vbs=4<cr>"
HKR, VoiceDialNumberSetup,      7,, "ats30=60<cr>"
HKR, GenerateDigit,             1,, "at#vts=<Digit><cr>"
HKR,, CallerIDPrivate,,P
HKR,, CallerIDOutSide,,O
HKR,, VariableTerminator,,<cr><lf>
HKR, EnableDistinctiveRing, 1,, "at+VDR=1,1<cr>"
HKR,, ForwardDelay,   1,88,13
HKR, Responses, "<cr><lf>VCON<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATE=", 1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "TIME=", 1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NMBR=", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NAME=", 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "MESG=", 1, 97, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>TIME=", 1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NMBR=", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NAME=", 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>MESG=", 1, 97, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING1<cr><lf>",        1, 18, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING2<cr><lf>",        1, 19, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING3<cr><lf>",        1, 1a, 00, 00,00,00,00, 00,00,00,00
HKR,, SpeakerPhoneSpecs,       1, 0A,00,00,00,  0f,00,00,00,  03,00,00,00,  00,00,00,00
HKR, SpeakerPhoneEnable,      1,, "at#cls=8<cr>"
HKR, SpeakerPhoneEnable,      2,, "at#vls=6<cr>"
HKR, SpeakerPhoneEnable,      3,, "at#spk=1,5,1<cr>"
HKR, SpeakerPhoneDisable,    1,, "at#spk=0,16,,<cr>"
HKR, SpeakerPhoneDisable,    2,, "at#vls=0<cr>"
HKR, SpeakerPhoneMute,        1,, "at#spk=0,,,<cr>"
HKR, SpeakerPhoneUnMute,      1,, "at#spk=1,,,<cr>"
HKR, SpeakerPhoneSetVolumeGain,  1,, "at#spk=,<Vol>,<Gain><cr>"
