;; netrtwlanu.inf 
;;
;; TP-LINK  Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2014 TP-LINK TECHNOLOGIES CO.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 03/31/2014,1026.9.0312.2014

[Manufacturer]
%Realtek% = Realtek, NTX86.5.1, NTamd64.5.1, NTX86.6.0, NTamd64.6.0, NTX86.6.1, NTamd64.6.1, NTX86.6.2, NTamd64.6.2, NTX86.6.3, NTamd64.6.3

[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTX86.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTamd64.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTX86.6.0]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTamd64.6.0]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTx86.6.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTamd64.6.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTX86.6.2]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTamd64.6.2]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTX86.6.3]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Realtek.NTamd64.6.3]
;; For 8192C RTK common		================================================================
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BFF&PID_8160								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176&REV_0200&SS
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177&REV_0200&SS
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170							; RTK 88CE_VAU board for B/G/N
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170&REV_0200&SS
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E						; RTK 88CE_VAU board for B/G
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E&REV_0200&SS
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C							; RTK 92CE_VAU board for B/G/N
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C&REV_0200&SS
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A						; RTK slim_solo board for B/G/N
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A&REV_0200&SS
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A					; LC slim solo for BGN.
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A&REV_0200&SS
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B					; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu8188RU.ndi,USB\VID_0BDA&PID_817F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu8188RU.ndi,USB\VID_0BDA&PID_817F&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F&REV_0200&SS
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A								; RTK 88RU board for B/G/N
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A&REV_0200&SS
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_103C&PID_1629								; HP/Liteon board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8192
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178								; RTK 92CU board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178&REV_0200&SS
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358								; AZ 88CE_VAU for B/G/N
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358&REV_0200&SS
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359							; AZ 88CE_VAU for B/G
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359&REV_0200&SS
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357								; AZ 88CUS for B/G/N
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357&REV_0200&SS
%RTL8188ctv.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_018A								; 8188CTV for BGN test only.

;; For 8192D RTK common		================================================================
%RTL8192du.DeviceDesc% 				= RTL8192du.ndi, 	USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%  			= RTL8192du.ndi, 	USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_8193&MI_01
%RTL8192du2.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_0193&MI_00
%RTL8192du3.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_0193&MI_01

;; For 8723 RTK common		================================================================
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_872B
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_8725&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0723&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_A724

;; For 8188E RTK common		================================================================
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179&REV_0200&SS
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179&REV_0200&SS
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179&REV_0200&SS

;; For 8812A RTK common		================================================================
%RTL8812au.DeviceDesc% 				= RTL8812au.ndi, 	USB\VID_0BDA&PID_8812
%RTL8812au_881A.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881A
;;%RTL8812au_881B.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881B
;;%RTL8812au_881C.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881C

;; For 8811A RTK common		================================================================
%RTL8811au.DeviceDesc% 				= RTL8811au.ndi, 	USB\VID_0BDA&PID_0811
%RTL8811au.DeviceDesc% 				= RTL8811au.ndi, 	USB\VID_0BDA&PID_A811
%RTL8811au.DeviceDesc% 				= RTL8811au.ndi, 	USB\VID_7392&PID_A813
%RTL8811au_Combo.DeviceDesc% 			= RTL8821auLC.ndi, 	USB\VID_0BDA&PID_0823&MI_02

;; For 8192E RTK common		================================================================
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818B
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818C&MI_02


;;----------------------------------------------------------------------------
;; For 8723B RTK common
;;----------------------------------------------------------------------------
%RTL8723bu.DeviceDesc% 				= RTL8723bu.ndi, 	USB\VID_0BDA&PID_B720&MI_02


;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------


[RTL8192cu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; 8188RU 8192cu installation
;;----------------------------------------------------------------------------



[RTL8192cu8188RU.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg, BeautifySignal.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu8188RU.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu8188RU.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------



[RTL8192cu_G.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, Ndis6UsbRxAgg.reg, TxByTimerOnn.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, 11gWirelessMode.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu_G.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192cu_G.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek N mode wake on wlan sku installation
;;----------------------------------------------------------------------------



[RTL8192cu_wow.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, Ndis6UsbRxAgg.reg, TxByTimerOnn.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, CIHVS.reg, WowlanAllEnableNoLPS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu_wow.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu_wow.ndi.NT.HW]
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.PnPFilterRegistration


;;----------------------------------------------------------------------------
;; Realtek 8192DU default installation
;;----------------------------------------------------------------------------



[RTL8192du.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, EDCCASupport.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8192du.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

[RTL8192du0.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du0.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du0.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8192du0.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

[RTL8192du1.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, ConcurrentMode.reg, 2G40MHzAnd5G40MHz.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du1.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du1.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du1.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; 92DU only 5G customized installation
;;----------------------------------------------------------------------------



[RTL8192du_5G.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg,BandOnly5G.reg, ScanType.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du_5G.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du_5G.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8192du_5G.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8723au default installation
;;----------------------------------------------------------------------------

             

[RTL8723au.ndi.NT]
AddReg				= NDIS_62.reg, RTL8723au.common.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, TimerGPIOSetting8723A.reg, WifiConfig.reg, PnpPreTransOn.reg , WowlanEnableNoLPSNoPatternMatch.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8723bu default installation
;;----------------------------------------------------------------------------

             

[RTL8723bu.ndi.NT]
AddReg				= NDIS_62.reg, RTL8723au.common.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, TimerGPIOSetting8723A.reg, WifiConfig.reg, PnpPreTransOn.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8188eu default installation
;;----------------------------------------------------------------------------



[RTL8188eu.ndi.NT]
AddReg				= NDIS_62.reg, RTL8188eu.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8811AU default installation
;;----------------------------------------------------------------------------



[RTL8811au.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




[RTL8821auLC.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg, WowlanEnableNoLPSNoPatternMatch.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821auLC.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821auLC.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration





[RTL8811au_PCI.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 5G11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au_PCI.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au_PCI.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8812AU default installation
;;----------------------------------------------------------------------------



[RTL8812au.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg, VHT24G.reg,HAdhoc.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8812au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812au_Vx.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, USBModeVx.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, ScanType.reg, WifiConfig.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71         ; IF_TYPE_IEEE80211
*MediaType			= 16         ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812au_Vx.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812au_Vx.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812au_Vx.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812auBelkin.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_Belkin.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auBelkin.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auBelkin.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




[RTL8812autplink.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, USBSwitch3.reg, WifiConfig.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812autplink.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812autplink.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8812autplink.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles





[RTL8812auDLink.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_DLink.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auDLink.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auDLink.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration
[RTL8812auDLink.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; NEC 8812AU default installation
;;----------------------------------------------------------------------------



[RTL8812auNEC.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, CustomerID_NEC.reg, NEC.reg, Signal.reg, sifs.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auNEC.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auNEC.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




[RTL8812auASUS.ndi.NT]
AddReg				= NDIS_62.reg, RTL8812au.common.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_ASUS.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auASUS.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auASUS.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;----------------------------------------------------------------------------
;; Realtek 8192E default installation
;;----------------------------------------------------------------------------



[RTL8192eu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, 11nWirelessMode.reg, RtlSsOff.reg,TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8192EU_COMMON.reg, TcpReorderEnable.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




;;
;; OS relative registry.
;;
[NDIS_62.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet, vwifi"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %RtlWlanu.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\RTWlanU.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"


;; For Different AC mode Rx parameters.
HKR,,AcUsbDmaTime,0,"10"
HKR,,AcUsbDmaSize,0,"5"
HKR,,AcUsbDmaTime2,0,"32"
HKR,,AcUsbDmaSize2,0,"5"

;; For IO mode switch.
HKR,,NByteAccess,0,"2"

;; For Init mode
HKR,,FWOffload,0,"2"


;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation OS Relative
;-------------------------------------------------------------------------------

[Ndis6UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"


[Ndis6UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

;;----------------------------------------------------------------------------
;; Wake on Wlan mode option parameters
;;----------------------------------------------------------------------------
[WowlanEnable.reg]
HKR,,WoWLANMode,0,"3"
HKR,,WoWLANLPSLevel,0,"1"

[WowlanDisable.reg]
HKR,,WoWLANMode,0,"0"
HKR,,WoWLANLPSLevel,0,"0"

[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANMode,0,"3"
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanEnableNoLPSNoPatternMatch.reg]
HKR,,WoWLANMode,0,"1"
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	PnP pre-transition handling
;-------------------------------------------------------------------------------
[PnpPreTransOn.reg]
HKR,,PreTransPnP,0,"1"
[PnpPreTransOff.reg]
HKR,,PreTransPnP,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"


;-------------------------------------------------------------------------------
;     Timer GPIO.
;-------------------------------------------------------------------------------
[TimerGPIOSettingCommon.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

[TimerGPIOSetting8723A.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

[TimerGPIOSetting8812AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"1"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;---------------------------------------------------------------------------------
;    Customer ID
;---------------------------------------------------------------------------------
[CustomerID_Belkin.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"22"

[CustomerID_DLink.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"44"

[CustomerID_NEC.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"45"

[CustomerID_ASUS.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"35"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;-------------------------------------------------------------------------------
;	Custom Tx Power Limit And Power By Rate Parameters
;-------------------------------------------------------------------------------
[CustomTxPwrConfigFile.reg]
HKR,,PwrByRateFile,0,""
HKR,,PwrLimitFile,0,""

;-------------------------------------------------------------------------------
; Intel Soft AP Mode Reg
;-------------------------------------------------------------------------------
[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"

;*******************************************************************************
; RTL8192du common paramters
;*******************************************************************************
[RTL8192du.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

;; For Earlymode 1:Enable 0:Disable
HKR,,bEarlymodeEnable,,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,SupportTxPacketBufferColease,0,"0"
HKR,,SupportTxPacketBufferColease,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"

HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"


;*******************************************************************************
; RTL8723au common paramters
;*******************************************************************************
[RTL8723au.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"1"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"


;*******************************************************************************
; RTL8812au common paramters
;*******************************************************************************
[RTL8188eu.common.reg]
;; For SoftApBss creator side judgement.
HKR,defaults,SoftApBss,0,"5"
HKR,,SoftApBss,0,"5"

;*******************************************************************************
; RTL8812au common paramters
;*******************************************************************************
[RTL8812au.common.reg]

;; For IQK Offload to FW.
HKR,,IQKFWOffload,0,"0"




;;----------------------------------------------------------------------------
;; LDPC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[LDPC_CONFIG.reg]
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "1",        0, "VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;;----------------------------------------------------------------------------
;; STBC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[STBC_CONFIG.reg]
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "2",        0, "VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;;----------------------------------------------------------------------------
;; Beamformer config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[BEAM_CONFIG.reg]
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "51"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "1",        0, "VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "2",        0, "VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"34"
HKR,,BeamformCap,0,"34"
HKR,,BeamformCap,,"34"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

;;Tx power limit
HKR,,EnableTxPowerLimit,0,"0"

;; For QoS test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\QoS,        ParamDesc,  0, "QoS Support"
HKR,Ndi\params\QoS,        type,       0, "enum"
HKR,Ndi\params\QoS,        default,    0, "0"
HKR,Ndi\params\QoS\enum,   "0",        0, "Not Support QoS"
HKR,Ndi\params\QoS\enum,   "1",        0, "Support QoS"
HKR,Ndi\params\QoS\enum,   "2",        0, "Auto"
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,,QoS,,"1"


HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------
HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"

HKR,defaults,RWRetry,0,"0"
HKR,,RWRetry,0,"0"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"
HKR,defaults,PwrByRate,0,"0"
HKR,,PwrByRate,0,"0"
HKR,defaults,PwrRaTbl1,0,"0"
HKR,,PwrRaTbl1,0,"0"
HKR,defaults,PwrRaTbl2,0,"0"
HKR,,PwrRaTbl2,0,"0"
HKR,defaults,PwrRaTbl3,0,"0"
HKR,,PwrRaTbl3,0,"0"
HKR,defaults,PwrRaTbl4,0,"0"
HKR,,PwrRaTbl4,0,"0"
HKR,defaults,PwrRaTbl5,0,"0"
HKR,,PwrRaTbl5,0,"0"
HKR,defaults,PwrRaTbl6,0,"0"
HKR,,PwrRaTbl6,0,"0"
HKR,defaults,PwrRaTbl7,0,"0"
HKR,,PwrRaTbl7,0,"0"
HKR,defaults,PwrRaTbl8,0,"0"
HKR,,PwrRaTbl8,0,"0"
HKR,defaults,PwrRaTbl9,0,"0"
HKR,,PwrRaTbl9,0,"0"
HKR,defaults,PwrRaTbl10,0,"0"
HKR,,PwrRaTbl10,0,"0"
HKR,defaults,PwrRaTbl11,0,"0"
HKR,,PwrRaTbl11,0,"0"
HKR,defaults,PwrRaTbl12,0,"0"
HKR,,PwrRaTbl12,0,"0"
HKR,defaults,PwrRaTbl13,0,"0"
HKR,,PwrRaTbl13,0,"0"
HKR,defaults,PwrRaTbl14,0,"0"
HKR,,PwrRaTbl14,0,"0"
HKR,defaults,PwrRaTbl15,0,"0"
HKR,,PwrRaTbl15,0,"0"
HKR,defaults,PwrRaTbl16,0,"0"
HKR,,PwrRaTbl16,0,"0"

HKR,defaults,GainOffsetFCCLow,0,"0"
HKR,,GainOffsetFCCLow,0,"0"
HKR,defaults,GainOffsetFCC,0,"0"
HKR,,GainOffsetFCC,0,"0"
HKR,defaults,GainOffsetFCCHigh,0,"0"
HKR,,GainOffsetFCCHigh,0,"0"

HKR,defaults,GainOffsetMKKLow,0,"0"
HKR,,GainOffsetMKKLow,0,"0"
HKR,defaults,GainOffsetMKK,0,"0"
HKR,,GainOffsetMKK,0,"0"
HKR,defaults,GainOffsetMKKHigh,0,"0"
HKR,,GainOffsetMKKHigh,0,"0"

HKR,defaults,GainOffsetETSILow,0,"0"
HKR,,GainOffsetETSILow,0,"0"
HKR,defaults,GainOffsetETSI,0,"0"
HKR,,GainOffsetETSI,0,"0"
HKR,defaults,GainOffsetETSIHigh,0,"0"
HKR,,GainOffsetETSIHigh,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

HKR,Ndi\params\EnableAdaptivity, 		ParamDesc, 	0, "EnableAdaptivity"
HKR,Ndi\params\EnableAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\EnableAdaptivity, 		default, 	0, "0"
HKR,Ndi\params\EnableAdaptivity\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"1", 		0, "Enable"
HKR,defaults,EnableAdaptivity, 0, "0"
HKR,,EnableAdaptivity, 0, "0"

[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

; Hw Beacon Max Error
HKR,,bBcnMaxErrorRegEnable,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

[NEC.reg]
HKR,Ndi\params\TxPwrPercentage, 	ParamDesc, 	0, %TX_PWR_CONTROL_STR%
HKR,Ndi\params\TxPwrPercentage, 	type, 		0, "enum"
HKR,Ndi\params\TxPwrPercentage, 	default, 	0, "8"
HKR,Ndi\params\TxPwrPercentage\enum, 	"1", 		0, %TX_PWR_PERCENTAGE_1_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"2", 		0, %TX_PWR_PERCENTAGE_2_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"4", 		0, %TX_PWR_PERCENTAGE_3_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"8", 		0, %TX_PWR_PERCENTAGE_4_STR%
HKR,defaults,TxPwrPercentage, 0, "8"
HKR,,TxPwrPercentage, 0, "8"

HKR,Ndi\params\StreamMode, 	ParamDesc, 	0, %STREAM_MODE_STR%
HKR,Ndi\params\StreamMode, 	type, 		0, "enum"
HKR,Ndi\params\StreamMode, 	default, 	0, "0"
HKR,Ndi\params\StreamMode\enum, 	"0", 		0, "OFF"
HKR,Ndi\params\StreamMode\enum, 	"1", 		0, "ON"
HKR,defaults,StreamMode, 0, "0"
HKR,,StreamMode, 0, "0"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

; /****************************************************************************
; ** Customerize Registry Area.
; ****************************************************************************/
[USBSwitch.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "0"
HKR,,ForcedUsbMode, 0, "0"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"10"
HKR,,UsbSwitchSpeed,0,"10"

HKR,defaults,UsbSwitchThL,0,"35"
HKR,,UsbSwitchThL,0,"35"

HKR,defaults,UsbSwitchThH,0,"45"
HKR,,UsbSwitchThH,0,"45"

HKR,defaults,UsbSwitchThRssi,0,"40"
HKR,,UsbSwitchThRssi,0,"40"

HKR,defaults,ViaU3,0,"0"
HKR,,ViaU3,0,"0"


HKR,defaults,ChannelPlan, 0, %CHNL_PLAN_VALUE%
HKR,,ChannelPlan, 0, %CHNL_PLAN_VALUE%

[USBSwitch3.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "8"
HKR,,ForcedUsbMode, 0, "8"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"50"
HKR,,UsbSwitchSpeed,0,"50"

HKR,defaults,UsbSwitchThL,0,"20"
HKR,,UsbSwitchThL,0,"20"

HKR,defaults,UsbSwitchThH,0,"5"
HKR,,UsbSwitchThH,0,"5"

HKR,defaults,UsbSwitchThRssi,0,"35"
HKR,,UsbSwitchThRssi,0,"35"

HKR,defaults,ViaU3,0,"0"
HKR,,ViaU3,0,"0"


HKR,defaults,ChannelPlan, 0, %CHNL_PLAN_VALUE%
HKR,,ChannelPlan, 0, %CHNL_PLAN_VALUE%

[USBModeVx.reg]
HKR,defaults,ForcedUsbMode, 0, "5"
HKR,,ForcedUsbMode, 0, "5"        

[Signal.reg]
HKR,defaults,LinkSpeedLevel, 0, "28"
HKR,,LinkSpeedLevel, 0, "28"

[BeautifySignal.reg]
HKR,Ndi\params\LinkSpeedLevel, 	ParamDesc, 	0, "Beautify Signal Strength Level"
HKR,Ndi\params\LinkSpeedLevel, 	type, 		0, "enum"
HKR,Ndi\params\LinkSpeedLevel, 	default, 	0, "0"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"0", 	0, "Default"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"52", 	0, "SS Display Lvl1"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"54", 	0, "SS Display Lvl2"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"56", 	0, "SS Display Lvl3"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"58", 	0, "SS Display Lvl4"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"60", 	0, "SS Display Lvl5"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"62", 	0, "SS Display Lvl6"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"64", 	0, "SS Display Lvl7"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"68", 	0, "SS Display Lvl8"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"70", 	0, "SS Display Lvl9"
HKR,defaults,LinkSpeedLevel, 0, "0"
HKR,,LinkSpeedLevel, 0, "0"


[sifs.reg]
HKR,defaults,SifsThresh, 0, "0"
HKR,,SifsThresh, 0, "0"


[ScanType.reg]
HKR,defaults,PassiveScan, 0, "0"
HKR,,PassiveScan, 0, "0"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c


;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,,BWSetting,0,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11agnWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,Ndi\params\WirelessMode\enum, 	"256", 		0, %IEEE_802_11AC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"10"
HKR,,RFType,0,"15"

HKR,,BWSetting,0,"2"

[5G11acWirelessMode.reg]
HKR,,WirelessMode, 0, "64"
HKR,,Channel,0,"36"
HKR,,RFType,0,"15"
HKR,,BWSetting,0,"2"

;;----------------------------------------------------------------------------
;; 11AC series IC VHT 2.4G Support
;;----------------------------------------------------------------------------
[VHT24G.reg]
;;HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G"
;;HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
;;HKR,Ndi\params\Vht24g, 		default, 	0, "0"
;;HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
;;HKR,Ndi\params\Vht24g\enum, 	"1", 		0, "Enable"
HKR,defaults,Vht24g, 0, "0"
HKR,,Vht24g, 0, "0"

;;----------------------------------------------------------------------------
;; 11N or higher Adhoc Mode
;;----------------------------------------------------------------------------
[HAdhoc.reg]
;;HKR,Ndi\params\11nAdhoc, 		ParamDesc, 	0, "High Adhoc Mode"
;;HKR,Ndi\params\11nAdhoc, 		type, 		0, "enum"
;;HKR,Ndi\params\11nAdhoc, 		default, 	0, "0"
;;HKR,Ndi\params\11nAdhoc\enum, 	"0", 		0, "Disable"
;;HKR,Ndi\params\11nAdhoc\enum, 	"1", 		0, "Enable"
HKR,defaults,11nAdhoc, 0, "0"
HKR,,11nAdhoc, 0, "0"

;;----------------------------------------------------------------------------
;; Usb selective suspend parameters
;;----------------------------------------------------------------------------
[NdisSS.reg]
HKR,Ndi\params\*SelectiveSuspend,	    ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,	    default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,	    type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,   "0",        0, "Disabled"
HKR,Ndi\params\*SelectiveSuspend\enum,   "1",        0, "Enabled"

HKR,Ndi\params\*SSIdleTimeout,	    ParamDesc,  0x00000020, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,	    type,       0x00000020, "int"
HKR,Ndi\params\*SSIdleTimeout,	    default,    0x00000020, "30"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0x00000020, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0x00000020, "5"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0x00000020, "1"

HKR,,*SSIdleTimeout, 0x00000020, "30"


;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; bandwidth setting
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"

[BandOnly5G.reg]
HKR,defaults,WirelessBand,0,"1"
HKR,,WirelessBand,0,"1"

;*****************************************************************************
; 92DU VS open EDCCA 
;*****************************************************************************
[EDCCASupport.reg]
HKR,defaults,EdccaSupport,0,"0"
HKR,,EdccaSupport,0,"0"


;*****************************************************************************
; For Wifi config
;*****************************************************************************
[WifiConfig.reg]
;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

;;----------------------------------------------------------------------------
;; 8811AU/8821AU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8811AU_COMMON.reg]
HKR,,EnableTxPowerLimit,0,"0"
HKR,,TxDutyEnable,0,"1"
HKR,,StbcCap,0,"17"
HKR,,RxSPStream,0,"1"
HKR,,RspPwr, 0, "1"

HKR,defaults,UsbTxAggDescNum,0,"10"
HKR,,UsbTxAggDescNum,0,"10"

HKR,,DecryptCustomFile,,"1"
HKR,,PwrByRateFile,0,"EncPWT.txt"
HKR,,PwrLimitFile,0,"TXPWR_LMT.txt"

HKR,,LdpcCap,0,"34"

HKR,,HWRTSEnable,,"1"

HKR,,BeamformCap,0,"34"

;;----------------------------------------------------------------------------
;; 8192EU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8192EU_COMMON.reg]
HKR,defaults,UsbTxAggDescNum,0,"15"
HKR,,UsbTxAggDescNum,0,"15"
HKR,,DisableBTCoexist,0,"1"
HKR,,WoWLANMode, 0, "0"

HKR,,LdpcCap,0,"0"
HKR,,StbcCap,0,"48"
HKR,,BeamformCap,0,"48"

HKR,,bEarlymodeEnable,0,"0"


;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
RTWlanU.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12
CoInstaller.CopyFiles = 11

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTWlanU.sys = 1
rtlCoInst.dll = 1
rtlCoInst.dat = 1

[SourceDisksNames]
1=%DISKNAME%,,,
[CoInstaller.AddReg]
HKR,,CoInstallers32,0x10000,"rtlCoInst.DLL,rtlCoInst"

[CoInstaller.CopyFiles]
rtlCoInst.dll,,,0x04
rtlCoInst.dat,,,0x04
;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHNL_PLAN_VALUE             = 127
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
AUTO_STR 				= "Auto"
IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
IEEE_802_11AC_STR			= "IEEE 802.11 ac"
SelectiveSuspend               		= "Selective suspend"
SSIdleTimeout                  		= "Selective suspend Timeout"

TX_PWR_CONTROL_STR		= "送信出力"
TX_PWR_PERCENTAGE_1_STR 	= "12.5%"
TX_PWR_PERCENTAGE_2_STR 	= "25%"
TX_PWR_PERCENTAGE_3_STR 	= "50%"
TX_PWR_PERCENTAGE_4_STR 	= "100%"
STREAM_MODE_STR			= "ストリーミングモード"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE		= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"


;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "TP-LINK TECHNOLOGIES CO."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX         			= "EDIMAX"
ELECOM         			= "ELECOM CO.,LTD."
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK					= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun					= "Shanghai Feixun Communication Co.,Ltd"
NetweeN					= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgear					= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."
HAWKING					= "Hawking Technologies Inc."
Compare					= "Compare Electronics CO.,LTD"
IO_DATA					= "I-O DATA DEVICE, INC"
TPLINK					= "TP-LINK Technologies Co."
Logitec					= "Logitec Japan"
NEC						= "NEC AccessTechnica, Ltd."
ACTIONTEC				= "Actiontec"
WD						= "Western Digital"
EnGenius				= "EnGenius Technologies."
Linksys					= "Linksys LLC"
BUFFALO					="BUFFALO INC."
Amped					= "Amped Wireless"

;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RtlWlanu.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RtlWlanu.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8192cu.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8192cu.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188cu.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8188cu.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188cu_G.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188ce_vau.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8188ce_vau.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8188ce_vau_G.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8188ce_vau_G.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8192ce_vau.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8192ce_vau.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_solo.DeviceDesc				= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_solo.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_solo_lc.DeviceDesc			= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_solo_lc.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_combo.DeviceDesc				= "TP-LINK Wireless USB Adapter"
RTL8188cu_slim_combo.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8188ru.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8188ru.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188cus_vl.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8188cus_vl.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTK_AZ88vau.DeviceDesc				= "TP-LINK Wireless USB Adapter"
RTK_AZ88vau.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTK_AZ88vau_G.DeviceDesc			= "TP-LINK Wireless USB Adapter"
RTK_AZ88vau_G.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTK_AZ88cus.DeviceDesc				= "TP-LINK Wireless USB Adapter"
RTK_AZ88cus.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188ctv.DeviceDesc				= "TP-LINK Wireless USB Adapter"
RTL8188ctv.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
PCI.DeviceDesc 						= "GW-USValue-EZ"
PCI.DeviceDesc.DispName				= "GW-USValue-EZ"
PCI-2.DeviceDesc 					= "GW-USLight"
PCI-2.DeviceDesc.DispName			= "GW-USLight"
PCI_Abocom88cu.DeviceDesc 			= "GW-USNano2"
PCI_Abocom88cu.DeviceDesc.DispName	= "GW-USNano2"
PCI_Abocom92cu.DeviceDesc 			= "GW-USEco300"
PCI_Abocom92cu.DeviceDesc.DispName	= "GW-USEco300"
PCI_Vencer.DeviceDesc 				= "BT-Micro3H2X Wireless LAN"
PCI_Vencer.DeviceDesc.DispName		= "BT-Micro3H2X Wireless LAN"
Sitecom.DeviceDesc 					= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom_UN.DeviceDesc 				= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_UN.DeviceDesc.DispName		= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_HG.DeviceDesc 				= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_HG.DeviceDesc.DispName		= "Wireless High-gain Network adapter 300N WLA-4001"
EDIMAX.DeviceDesc 					= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX.DeviceDesc.DispName			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX300.DeviceDesc 				= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
Abocom.DeviceDesc 					= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Amigo.DeviceDesc 					= "Wireless USB Card"
Amigo.DeviceDesc.DispName			= "Wireless USB Card"
Hercules.DeviceDesc 				= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
Hercules-E035.DeviceDesc 			= "Hercules Wireless N Mini v2 USB Key"
Hercules-E035.DeviceDesc.DispName	= "Hercules Wireless N Mini v2 USB Key"
DLink-1.DeviceDesc 					= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 					= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 					= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-4.DeviceDesc 					= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-4.DeviceDesc.DispName			= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-5.DeviceDesc 					= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
DLink-5.DeviceDesc.DispName			= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
Belkin.DeviceDesc 					= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName			= "Surf Wireless Micro USB Adapter"
Belkin-2.DeviceDesc 				= "Belkin Surf & Share Wireless USB Adapter"
Belkin-2.DeviceDesc.DispName		= "Belkin Surf & Share Wireless USB Adapter"
Belkin-3.DeviceDesc 				= "N300 USB Network Adapter"
Belkin-3.DeviceDesc.DispName		= "N300 USB Network Adapter"
Belkin-4.DeviceDesc 				= "Belkin Wireless Adapter"
Belkin-4.DeviceDesc.DispName		= "Belkin Wireless Adapter"
ZyXEL.DeviceDesc 					= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ATKK.DeviceDesc						= "Corega CG-WLUSB300NS"
ATKK.DeviceDesc.DispName			= "Corega CG-WLUSB300NS"
TRENDnet.DeviceDesc					= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet.DeviceDesc.DispName		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet_2.DeviceDesc				= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_2.DeviceDesc.DispName		= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
Feixun.DeviceDesc 					= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun.DeviceDesc.DispName			= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc 					= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc.DispName			= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
XAVI.DeviceDesc 					= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI.DeviceDesc.DispName			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI88cusc.DeviceDesc 				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
XAVI88cusc.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
Netgear.DeviceDesc 					= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Netgear.DeviceDesc.DispName			= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Oar_Inc.DeviceDesc 					= "SW-WF02-AD15"
Oar_Inc.DeviceDesc.DispName			= "SW-WF02-AD15"
ASUS.DeviceDesc 					= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS.DeviceDesc.DispName			= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc 					= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc.DispName			= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-17C0.DeviceDesc 				= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
ASUS-17C0.DeviceDesc.DispName		= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
Hawking-1.DeviceDesc 				= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-1.DeviceDesc.DispName		= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-2.DeviceDesc 				= "Hawking HWUN4 Wls-300N Adapter"
Hawking-2.DeviceDesc.DispName		= "Hawking HWUN4 Wls-300N Adapter"
Compare-1.DeviceDesc 				= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
Compare-1.DeviceDesc.DispName		= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
IO_DATA_094c.DeviceDesc				= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_094c.DeviceDesc.DispName	= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc				= "I-O DATA WN-G300UA Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc.DispName	= "I-O DATA WN-G300UA Wireless LAN Adapter"
TPLINK-0100.DeviceDesc				= "300Mbps Wireless High Power USB Adapter"
TPLINK-0100.DeviceDesc.DispName		= "300Mbps Wireless High Power USB Adapter"
Logitec_016D.DeviceDesc				= "Logitec LAN-WH300NU2 LAN Adapter"
Logitec_016D.DeviceDesc.DispName	= "Logitec LAN-WH300NU2 LAN Adapter"

;*******************************************************************************
; RTL8192DU Device description
;*******************************************************************************
RTL8192du.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8192du.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8192du0.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8192du0.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8192du1.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8192du1.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8192du2.DeviceDesc           	= "TP-LINK Wireless USB Adapter"
RTL8192du2.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8192du3.DeviceDesc           	= "TP-LINK Wireless USB Adapter"
RTL8192du3.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
PCI_Abocom_du0.DeviceDesc 			= "GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName	= "GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc 			= "GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName	= "GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc 				= "GW-USFang300 MAC0"
PCI_3_du0.DeviceDesc.DispName		= "GW-USFang300 MAC0"
PCI_3_du1.DeviceDesc 				= "GW-USFang300 MAC1"
PCI_3_du1.DeviceDesc.DispName		= "GW-USFang300 MAC1"
PCI_4_du0.DeviceDesc 				= "GW-USUltra300 MAC0"
PCI_4_du0.DeviceDesc.DispName		= "GW-USUltra300 MAC0"
PCI_4_du1.DeviceDesc 				= "GW-USUltra300 MAC1"
PCI_4_du1.DeviceDesc.DispName		= "GW-USUltra300 MAC1"
PCIWIDI_92DU.DeviceDesc 			= "MZK-WD300DH"
PCIWIDI_92DU.DeviceDesc.DispName	= "MZK-WD300DH"
Abocom_92DU0.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU0.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU1.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_92DU1.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_AB33.DeviceDesc				= "GW-300S KATANA"
Abocom_AB33.DeviceDesc.DispName		= "GW-300S KATANA"
Abocom_818B.DeviceDesc				= "Wireless LAN 802.11n USB2.0 Network Adapter"
Abocom_818B.DeviceDesc.DispName		= "Wireless LAN 802.11n USB2.0 Network Adapter"
Belkin-N600DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N600DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
DLink-DWA151.DeviceDesc                 = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"   
DLink-DWA151.DeviceDesc.DispName        = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"  
TRENDnet_3_du.DeviceDesc			= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc.DispName	= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
Logitec.DeviceDesc					= "150N 5GHz USB Dongle"
Logitec.DeviceDesc.DispName			= "150N 5GHz USB Dongle"
EDIMAX5G.DeviceDesc			= "RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"
EDIMAX5G.DeviceDesc.DispName		= "RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"
ScreenBeam.DeviceDesc 				= "Actiontec ScreenBeam USB Transmitter"
ScreenBeam.DeviceDesc.DispName		= "Actiontec ScreenBeam USB Transmitter"
;*******************************************************************************
; RTL8723au Device description
;*******************************************************************************
RTL8723au.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8723au.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
;*******************************************************************************
; RTL8723bu Device description
;*******************************************************************************
RTL8723bu.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8723bu.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8188eu.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8188ee_vau.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8188ee_vau.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
RTL8188eu_0179.DeviceDesc 			= "TP-LINK Wireless USB Adapter"
RTL8188eu_0179.DeviceDesc.DispName	= "TP-LINK Wireless USB Adapter"
Abocom_8179.DeviceDesc 				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom_8179.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
DLINK_330F.DeviceDesc 				= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_330F.DeviceDesc.DispName		= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc 				= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc.DispName		= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3311.DeviceDesc 				= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
DLINK_3311.DeviceDesc.DispName		= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
;*******************************************************************************
; RTL8812AU Device description
;*******************************************************************************
RTL8812au.DeviceDesc 					= "TP-LINK Wireless USB Adapter"
RTL8812au.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"
RTL8812au_881A.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8812au_881A.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8812au_881B.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8812au_881B.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"
RTL8812au_881C.DeviceDesc 				= "TP-LINK Wireless USB Adapter"
RTL8812au_881C.DeviceDesc.DispName		= "TP-LINK Wireless USB Adapter"

Belkin-AC950.DeviceDesc					= "Belkin USB Wireless Adapter"
Belkin-AC950.DeviceDesc.DispName		= "Belkin USB Wireless Adapter"

Netgear-A6200v2.DeviceDesc              = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"
Netgear-A6200v2.DeviceDesc.DispName     = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"

DLink-DWA183.DeviceDesc                 = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA183.DeviceDesc.DispName        = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA182.DeviceDesc                 = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink-DWA182.DeviceDesc.DispName        = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink_3315.DeviceDesc                	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3315.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc                 	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"

Edimax_A822.DeviceDesc 				= "Edimax AC1200 Wireless LAN USB Adapter"
Edimax_A822.DeviceDesc.DispName		= "Edimax AC1200 Wireless LAN USB Adapter"

Sitecom_0074.DeviceDesc 				= "Sitecom WiFi USB adapter AC1200"
Sitecom_0074.DeviceDesc.DispName		= "Sitecom WiFi USB adapter AC1200"

Sitecom_007A.DeviceDesc 				= "WiFi High Gain USB Adapter AC600"
Sitecom_007A.DeviceDesc.DispName		= "WiFi High Gain USB Adapter AC600"

IO_DATA_0952.DeviceDesc					= "I-O DATA WN-AC867U Wireless LAN Adapter"
IO_DATA_0952.DeviceDesc.DispName		= "I-O DATA WN-AC867U Wireless LAN Adapter"
                                    	
Logitec_016E.DeviceDesc					= "Logitec AC866 Wireless USB Adapter"
Logitec_016E.DeviceDesc.DispName		= "Logitec AC866 Wireless USB Adapter"
                                    	
ASUS_17D2.DeviceDesc 					= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
ASUS_17D2.DeviceDesc.DispName			= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
                                    	
Hawking_0022.DeviceDesc 				= "Hawking USB Wireless-AC Network Adapter"
Hawking_0022.DeviceDesc.DispName		= "Hawking USB Wireless-AC Network Adapter"

NEC_0408.DeviceDesc						= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"
NEC_0408.DeviceDesc.DispName			= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"

Zyxel_3426.DeviceDesc					= "ZyXEL Wireless AC USB Adapter"
Zyxel_3426.DeviceDesc.DispName			= "ZyXEL Wireless AC USB Adapter"

WD_0632.DeviceDesc						= "WD My Net AC USB Adapter"
WD_0632.DeviceDesc.DispName				= "WD My Net AC USB Adapter"

EnGenius_0100.DeviceDesc				= "EnGenius 802.11ac Dual Band Wireless USB Adapter"
EnGenius_0100.DeviceDesc.DispName		= "EnGenius 802.11ac Dual Band Wireless USB Adapter"

Linksys_003F.DeviceDesc					= "Linksys WUSB6300"
Linksys_003F.DeviceDesc.DispName		= "Linksys WUSB6300"

Amped_9097.DeviceDesc					= "Amped Wireless ACA1 Wi-Fi Adapter"
Amped_9097.DeviceDesc.DispName			= "Amped Wireless ACA1 Wi-Fi Adapter"

TPLINK_0101.DeviceDesc					= "TP-LINK Wireless USB Adapter"
TPLINK_0101.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"

PCI_AB30.DeviceDesc 				= "GW-900D"
PCI_AB30.DeviceDesc.DispName		= "GW-900D"

Abocom_8812.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_8812.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"

Abocom_0811.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_0811.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"

TRENDnet_805B.DeviceDesc 			= "AC1200  Dual Band Wireless USB Adapter"
TRENDnet_805B.DeviceDesc.DispName		= "AC1200  Dual Band Wireless USB Adapter"

Buffalo_025D.DeviceDesc				= "BUFFALO WI-U3-866D Wireless LAN Adapter"
Buffalo_025D.DeviceDesc.DispName		= "BUFFALO WI-U3-866D Wireless LAN Adapter"

;*******************************************************************************
; RTL8811AU Device description
;*******************************************************************************
RTL8811au.DeviceDesc					= "TP-LINK Wireless USB Adapter"
RTL8811au.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"
RTL8811au_Combo.DeviceDesc					= "TP-LINK Wireless USB Adapter"
RTL8811au_Combo.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"

Buffalo-WI-U2-433DM.DeviceDesc 						= "BUFFALO WI-U2-433DM Wireless LAN Adapter"
Buffalo-WI-U2-433DM.DeviceDesc.DispName 		= "BUFFALO WI-U2-433DM Wireless LAN Adapter"

Edimax_AC600.DeviceDesc					= "Edimax AC600 Wireless LAN USB Adapter"
Edimax_AC600.DeviceDesc.DispName		= "Edimax AC600 Wireless LAN USB Adapter"

ELECOM_WDC433DU2.DeviceDesc				= "ELECOM WDC-433DU2H 11ac Wireless Adapter"
ELECOM_WDC433DU2.DeviceDesc.DispName	= "ELECOM WDC-433DU2H 11ac Wireless Adapter"

ELECOM_4009.DeviceDesc				= "ELECOM WDC-300SU2S Wireless Adapter"
ELECOM_4009.DeviceDesc.DispName		= "ELECOM WDC-300SU2S Wireless Adapter"

ELECOM_4008.DeviceDesc				= "ELECOM WDC-150SU2M Wireless Adapter"
ELECOM_4008.DeviceDesc.DispName		= "ELECOM WDC-150SU2M Wireless Adapter"

Hawking_0023.DeviceDesc					= "Hawking USB WLS 11AC Adapter"
Hawking_0023.DeviceDesc.DispName		= "Hawking USB WLS 11AC Adapter"

IO_DATA_AC433UA.DeviceDesc					= "I-O DATA WN-AC433UA Wireless LAN Adapter"
IO_DATA_AC433UA.DeviceDesc.DispName		= "I-O DATA WN-AC433UA Wireless LAN Adapter"

DLink-DWA171.DeviceDesc	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink-DWA171.DeviceDesc.DispName	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink_3318.DeviceDesc	=	 "D-Link DWA-172 Wireless AC600 Dual Band USB Adapter with Signal Plus"
DLink_3318.DeviceDesc.DispName	=	 "D-Link DWA-172 Wireless AC600 Dual Band USB Adapter with Signal Plus"

TRENDnet_804B.DeviceDesc	=	 "AC600 Dual Band Wireless USB Adapter"
TRENDnet_804B.DeviceDesc.DispName	=	 "AC600 Dual Band Wireless USB Adapter"


PCI_AB32.DeviceDesc					=	"GW-450S"
PCI_AB32.DeviceDesc.DispName		=	"GW-450S"
;*******************************************************************************
; RTL8192E Device description
;*******************************************************************************
RTL8192eu.DeviceDesc					= "TP-LINK Wireless USB Adapter"
RTL8192eu.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"
DLink_2001.DeviceDesc				= "D-Link DWA-131 Wireless N Nano USB Adapter"
DLink_2001.DeviceDesc.DispName		= "D-Link DWA-131 Wireless N Nano USB Adapter"

