;/*++
;
;Module Name:
;
;    netathuwx.inf
;
;    Installs athuw.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs athuwx.sys (NDIS 5 driver) on 9x platforms
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
Compatible  = 1
DriverVer   = 07/28/2011,7.7.0.102
Catalogfile.nt = netathuwx.cat

[Manufacturer]
%ATHEROS%     = Atheros, NTX86.5.1, NTamd64.5.1, NTX86.6.0, NTamd64.6.0, NTX86.6.1, NTamd64.6.1

[ControlFlags]
ExcludeFromSelect = *

[Atheros]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Atheros.NTX86.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Atheros.NTamd64.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ATHER.DeviceDesc.9271% = ATHER_DEV_9271.ndi,     USB\VID_0CF3&PID_9271
;%ATHER.DeviceDesc.7010% = ATHER_DEV_7010.ndi,     USB\VID_0CF3&PID_7010
%ATHER.DeviceDesc.7015% = ATHER_DEV_7015.ndi,     USB\VID_0CF3&PID_7015
;%ATHER.DeviceDesc.1006% = ATHER_DEV_1006.ndi,     USB\VID_0CF3&PID_1006

[Atheros.NTX86.6.0]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Atheros.NTamd64.6.0]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Atheros.NTX86.6.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

[Atheros.NTamd64.6.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------

; Windows NT specific entries
[ATHER_DEV_9271.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, wpsBtnSupport.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_9271.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7010.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd.reg, 7010.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7010.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7015.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg, wpsBtnSupport.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7015.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1006.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, customer1.SCAN.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1006.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog



;AMD 64
; Windows AMD64 specific entries

[ATHER_DEV_9271.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg,ATHR_9271.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_9271.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7010.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd.reg, 7010.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7010.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7015.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg, wpsBtnSupport.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7015.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1006.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgub.reg, uapsd.reg,ATHR_9271.reg, customer1.SCAN.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1006.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;===========================CUSTOM SECTION=====================================
; Windows NT specific entries
[NTGR_DEV_9030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, NTGR.reg, scanReduce.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[NTGR_DEV_9030.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries

[NTGR_DEV_9030.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg,ATHR_9271.reg, NTGR.reg, scanReduce.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[NTGR_DEV_9030.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

; Windows NT specific entries
[NTGR_DEV_9018.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd_VO.reg, NTGR_9018.reg, htDisableWepTkip.reg, scanReduce.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[NTGR_DEV_9018.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries

[NTGR_DEV_9018.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd_VO.reg, NTGR_9018.reg, htDisableWepTkip.reg, scanReduce.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[NTGR_DEV_9018.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[DLINK_DEV_3A10.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, DLINK.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[DLINK_DEV_3A10.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries

[DLINK_DEV_3A10.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg,ATHR_9271.reg, DLINK.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[DLINK_DEV_3A10.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3327.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3327.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3327.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3327.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3328.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3328.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3328.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3328.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3346.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3346.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3346.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3346.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3348.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3348.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3348.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3348.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3349.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3349.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3349.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3349.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[AZWV_DEV_3350.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3350.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries
[AZWV_DEV_3350.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[AZWV_DEV_3350.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[SMC_DEV_A704.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[SMC_DEV_A704.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;AMD 64
; Windows AMD64 specific entries

[SMC_DEV_A704.ndi.NTamd64]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[SMC_DEV_A704.ndi.NTamd64.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

;===========================CUSTOM SECTION END=================================

;
; 5416 Enumerated Types
;

[5416.bgub.reg]
HKR, ,                                  NetBand,                        0x00002,  "12"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"

[5416.bgnub.reg]
HKR, ,                                  NetBand,                        0x00002,  "40972"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"

[5416.abgnub.reg]
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "61455"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "61455",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "20481",                        0,  %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "40972",                        0,  %WirelessMode2GHzOnly%

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainSelect,                 	0x00002,  "7"
;HKR, ,                                  txChainSelectLegacy,            0x00002,  "5"
HKR, ,                                  rxChainSelectLegacy,           	0x00002,  "7"
HKR, ,                                  forceBias,           	        0x00002,  "2"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1823"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1823",                         0,        %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "1795",                         0,        %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "28",                           0,        %WirelessMode2GHzOnly%

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                 	0x00002,  "0"

[d3hot.reg]
HKR, ,                                  pciePowerReset,                 0x00002,  "0"
HKR, ,                                  pcieRestore,                 	0x00002,  "1"

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

; Allow non admin uses to switch profiles
;[5211.reg.security]
;"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnable,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnable,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnable,            default,                        0,  "0"
HKR, Ndi\params\psPollEnable,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnable\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnable\enum,       "0",                            0,  %psPollDisable%

[uapsd_VO.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "1"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnable,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnable,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnable,            default,                        0,  "1"
HKR, Ndi\params\psPollEnable,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnable\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnable\enum,       "0",                            0,  %psPollDisable%

;-----------------------------------------------------------------------------
;
; 5416 common
;
[5416.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,rmEnable
HKR,,overrideACstatus
HKR, Ndi\params\NetBand
HKR,,rxChainSelect
HKR,,txChainSelectLegacy
HKR,,rxChainSelectLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,pciePowerSaveEnable
HKR,,pcieAspm
HKR,,scanReduceLevel
HKR,,scanTimePreSleep
HKR,,wpsButtonGpio
HKR,,wpsBtnSupport

[5416.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "0"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, Ndi\params\PSPXLinkMode,           ParamDesc,                      0,  %PSPXLinkMode%
HKR, Ndi\params\PSPXLinkMode,           Base,                           0,  "10"
HKR, Ndi\params\PSPXLinkMode,           default,                        0,  "0"
HKR, Ndi\params\PSPXLinkMode,           type,                           0,  "enum"
HKR, Ndi\params\PSPXLinkMode\enum,      "1",                            0,  %PSPXLinkModeEnable%
HKR, Ndi\params\PSPXLinkMode\enum,      "0",                            0,  %PSPXLinkModeDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[7010.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002, "1"
HKR, ,                                  htAdhocEnable,                   0x00002, "0"
HKR, ,                                  isMagpie,                        0x00002, "1"
HKR, ,                                  gpioLedCustom,                   0x00002, "1"
HKR, ,                                  gpioPinFunc0,                    0x00002, "12"
HKR, ,                                  gpioPinFunc1,                    0x00002, "10"
HKR, ,                                  stbcEnable,                      0x00002, "1"
HKR, ,                                  wpsButtonGpio,                   0x00002, "13"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"

[7015.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002, "1"
HKR, ,                                  htAdhocEnable,                   0x00002, "0"
HKR, ,                                  isMagpie,                        0x00002, "1"
HKR, ,                                  gpioLedCustom,                   0x00002, "1"
HKR, ,                                  gpioPinFunc0,                    0x00002, "12"
HKR, ,                                  gpioPinFunc1,                    0x00002, "10"
HKR, ,                                  stbcEnable,                      0x00002, "1"
HKR, ,                                  wpsButtonGpio,                   0x00002, "4"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"

[htDisableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                 0x00002, "0"

[wpsBtnSupport.reg]
HKR, ,                                  wpsBtnSupport,                   0x00002, "1"

[surpriseRemovalOk.reg]
HKR, ,                                  surpriseRemovalOk,               0x10003, 1

[scanReduce.reg]
HKR, ,                                  scanReduceLevel,                 0x00002, "1"
HKR, ,                                  scanTimePreSleep,                0x00002, "10"

[NTGR.reg]
HKR, ,                                  ignore11dBeacon,                0, 1
HKR, ,                                  gpioLedCustom,                  0, 8
HKR, ,                                  gpioPinFunc0,                   0, 15
HKR, ,                                  swapDefaultLED,                 0, 1
HKR, ,                                  GreenTx,                        0, 15
HKR, ,                                  htEnableWepTkip,          0x00002, "3"
HKR, ,                                  htEnableWepTkipAgg,       0x00002, "0"

[NTGR_9018.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002, "1"
HKR, ,                                  htAdhocEnable,                   0x00002, "0"
HKR, ,                                  isMagpie,                        0x00002, "1"
HKR, ,                                  gpioLedCustom,                   0x00002, "9"
HKR, ,                                  gpioPinFunc0,                    0x00002, "12"
HKR, ,                                  gpioPinFunc1,                    0x00002, "10"
HKR, ,                                  GreenTx,                         0, 0
HKR, ,                                  updatelinkspeed,                 0, 1
HKR, ,                                  pciePowerSaveEnable,             0, 2
HKR, ,                                  stbcEnable,                      0x00002, "1"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"

[DLINK.reg]
HKR, , gpioLedCustom,   0, 1
HKR, , gpioPinFunc0,    0, 15
HKR, , swapDefaultLED,  0, 1
;-----------------------------------------------------------------------------
;;Customized Section

[customer0.reg]
;PCIe Related
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR,,                 isMagpie,                 0, 0
[customer0.LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0.LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[customer1.SCAN.reg]
HKR, ,                                  bkPeriodicScanEnable,           0x00002,  "0"
HKR, ,                                  scanPendingCriterion,           0x00002,  "65"

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "49719"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "32772",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "16387",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "32796",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "49719",                        0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "2075"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "2075",                         0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "0"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchAuto%

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR9271"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"

[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\athuwx.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; System TCPIP parameter changes
;
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

[sys.TcpParamslan.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

;----------------------------------------------------------------------------
;*********************************************************************
;   Atheros Client Installation Program
;*********************************************************************
[ATHR_9271.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002,  "1"
HKR, ,                                  htAdhocEnable,                   0x00002,  "0"
HKR, ,                                  wpsButtonGpio,                   0x00002,  "13"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
athuwx.sys,,,2

[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %Atheros_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
athuwx.sys                   = 1,, ; on distribution disk 1


[DestinationDirs]
ATHER.CopyFiles.nt           = 12
;ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
Atheros                      = "TP-LINK"
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
scanTimeValid                = "Scan Valid Interval"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
WirelessMode                 = "Wireless Mode Selection"
WirelessModeAuto             = "Auto"
WirelessMode5GHzOnly         = "5 GHz Only"
WirelessMode2GHzOnly         = "2.4 GHz Only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryLow            = "Very Low"
roamPolicyLow                = "Low"
roamPolicyNormal             = "Normal"
roamPolicyHigh               = "High"
roamPolicyVeryHigh           = "Very High"
scanTimeValidcust            = "Roam Time (sec)"
scanTimeValidcust120         = "120"
scanTimeValidcust60          = "60"
scanTimeValidcust45          = "45"
scanTimeValidcust30          = "30"
scanTimeValidcust20          = "20"
scanTimeValidcust10          = "10"
scanTimeValidcust5           = "5"
sleepMode_DEFAULT            = "2"  
NetBand_DEF_STR_A            = "3"                       ; (A/T) 
NetBand_DEF_STR_AB           = "7"                       ; (A/T/B)   
NetBand_DEF_STR_G            = "12"                      ; (B/G)     
NetBand_DEF_STR_AG           = "15"                      ; (A/T/B/G)
AdhocBand_DEF_STR_A          = "1"                       ; (A)
AdhocBand_DEF_STR_AB         = "1"                       ; (A)
AdhocBand_DEF_STR_G          = "0"                       ; (B)
AdhocBand_DEF_STR_AG         = "0"                       ; (B)
shortPreamble_DEFAULT        = "1"
authTypeUseOnly              = "802.11 Authentication Type"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledVI               = "Power Save Policy (Video)"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVIOff            = "Legacy Power Save"
uapsdEnabledVO               = "Power Save Policy (Voice)"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVOOff            = "Legacy Power Save"
psPoll                       = "Power Save Legacy Algorithm"
psPollEnable                 = "PS Poll"
psPollDisable                = "PS non Poll"
ccx5FeatureEnable            = "MFP"
ccx5FeatureEnableMfpEnable   = "Enable"
ccx5FeatureEnableMfpDisable  = "Disable"
Mode11d                      = "11d Mode Switch"
Mode11dEnable                = "Enable"
Mode11dDisable               = "Disable"
RateCtrl                     = "Auto Transmit Rate"
RateCtrlEnable               = "Enable"
RateCtrlDisable              = "Disable"
TxRate11b                    = "11b Transmit Rates"
TxRate11b1M                  = "1 Mbps"
TxRate11b2M                  = "2 Mbps"
TxRate11b5M                  = "5.5 Mbps"
TxRate11b11M                 = "11 Mbps"
TxRate11g                    = "11g Transmit Rates"
TxRate11g1M                  = "1 Mbps"
TxRate11g2M                  = "2 Mbps"
TxRate11g5M                  = "5.5 Mbps"
TxRate11g11M                 = "11 Mbps"
TxRate11g6M                  = "6 Mbps"
TxRate11g9M                  = "9 Mbps"
TxRate11g12M                 = "12 Mbps"
TxRate11g18M                 = "18 Mbps"
TxRate11g24M                 = "24 Mbps"
TxRate11g36M                 = "36 Mbps"
TxRate11g48M                 = "48 Mbps"
TxRate11g54M                 = "54 Mbps"
TxRate11a                    = "11a Transmit Rates"
TxRate11a6M                  = "6 Mbps"
TxRate11a9M                  = "9 Mbps"
TxRate11a12M                 = "12 Mbps"
TxRate11a18M                 = "18 Mbps"
TxRate11a24M                 = "24 Mbps"
TxRate11a36M                 = "36 Mbps"
TxRate11a48M                 = "48 Mbps"
TxRate11a54M                 = "54 Mbps"
ATHR_VID_0CF3                = "VID_0CF3"
NTGR_VID_0846                = "VID_0846"
AZWV_VID_13D3                = "VID_13D3"
LION_VID_04CA                = "VID_04CA"
PSPXLinkMode                 = "PSP XLink mode"
PSPXLinkModeEnable           = "Enable"
PSPXLinkModeDisable          = "Disable"

Atheros_Disk                 = "Driver Disk 1"
ATHER.Service.DispName       = "Wireless Network Adapter Service"
ATHER.DeviceDesc.9271        = "TP-LINK Wireless USB Adapter"
ATHER.DeviceDesc.7015        = "TP-LINK Wireless USB Adapter"