1.  install OPOS_CCOs_1.13.001.msi first.
    for more infomation about the opos ccos please goto  http://monroecs.com/oposccos_current.htm

2.  install nlsoposinstall.msi, this is the newland auto-id opos service object for newland scanner.

* if you select the serial port as the communication type, please set 
	Baud rate=9600
	Data bits=8
	Parity bit=None
	Stop bit=1


Release note:
Release date:2011-12-23
Support device:NLS_EM1300/NLS_EM2028/NLS_EM3000/NLS_FM100/NLS_FM420/NLS_HR100/NLS_HR200

