Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
E_PO_CV2
E value converter DC supply positive converter 2: E2Q100X1:18 - EZX34:18 - EZ130X1:A26 no input to EZ130 version 4512 108 08661..4 release 2 generators release 3 generators only with 2 converters EZ130 version 4512 108 09102...4 0...+12V = 0...+375V if converter is stand-alone (E2Q X1 not connected) if in normal operation: E_PO + E_NG >> 445VDC = 10V measuring input EZ130 X1:A26 - X1:C26