### (1) Film.tdl

If the film type is not in the default data list, then select one of the film files:
FILM_BL.TDL (blue), FILM_GR.TDL (green), FILM_UV.TDL (ultra violet).
Select the one which matches the sensitivity factor S and RLF compensation.
S is a multiplication factor for the speed type of the screen:

If the screen = 400 and S_film = 0.5, then the total system is 200.

PCR: Select from FILM.TDL: X-CONSTANT RLF=1
DiDi: Select from FILMFSX.TDL: PHIL.Tri-FSXD