Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Communications check with EZ139
Start a communications program (PROCOMM), connect a data cable (no null modem) to EZ139 and set the port settings to: 9600 baud 8 data bits no parity 2 stop bits none protocol parity check off emulation ANSI (if asked) Turn the generator on or push the reset button to boot the Central unit. The following string should come up at the PC screen. 'þþþþþþþþÿþþþÿøþþÿþþþþþþþþþþÿþÿÿþþþÿÿÿÿÿþþÿþÿ ;I,"XRG90 CU Startup - Proms are R3V1L3 on 24-06-98 at 16 LSB 6882 MSB A022".;H,"Ready for Communication". Now push the "." key on the service PC, the following error message string should appear: ;E,"Syntax error: Route definition".;I,"ERROR Task No: 11700 Proc No: 11503 Error No: SQ".;I,"Task : T_SE_main Proc : SE_get_node_ID".;I,"Cause : PCcomm: Syntax error in node ID".;I,"".;E,"ERROR: 00SQ PCcomm: Syntax error in node ID".