### Disable Tube

If a tube (e.g. 2nd tube) shall be removed from a system one should use this function.

If a tube shall be removed temporarily one should do it at the registration device ‘RGDV1...8 Data Set A’.

In combination with ‘Bucky Ctrl. 1/Dig.Diag.’: DO NOT use this function before all RGDV associated to have been changed to ‘none’ instead of ‘Bucky Ctrl. 1/Dig.Diag.’.

- This function must be used if a double focus tube shall be replaced by a single focus tube.
- The non-used small filament circuit of FU_mA must be switched off.

- If a double focus tube shall be replaced by any other type, it is not required to disable the tube.
- Just load the other tube type according to ‘Tube 1...3 Data Set’.