Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00TC | Error |
Description:
TTS (Tube Temperature Supervision): Internal TTS Error
Possible Causes / Advice:
tube data table corrupted? Can happen after CU Complete restore if tubes are of a different speed type. Reboot generator to get it into a stable standby condition, then repeat loading of CU Complete. If error persistent even after reboot erase NV-RAM perform the Memory Quick Erase and start programming from scratch.