Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
PO_26V_RE
+ 26 V reverse supply EWAW11 - EWAW12 - EWAX1/2/3/4:4 - EWAX42:1 if generator and system release voltages don't match normal condition: PO_26V_RE = +26V of generator against ground (jumper WA W11 + W13 closed, W12 open) special condition: PO_26_RE = 0V against -24V, supply from stand (jumper WA W11 + W13 open, W12 closed)