Tube adaption OMTC TheBox

Warning! Radiation is released during the procedure

The door of the exam. room must be closed.

The collimator of the selected tube must be closed.

The II should be protected against X-ray with a lead apron.

If possible release the exposures from a radiation protected area.

After Tube installation (replacement) switch over to the TCOP Servicesoftware.

Select:

RUN/ ADJUSTMENT / Start adjust / GENERATOR / ADAPTION

Select the Focus you want to adapt.

Start the adjustment procedure by pressing the handswitch (footswitch) until the digit "1" appears.

The next step "Boost Adaptation" has to be carried out until a "tube dependent" value appears.

The last step "Boost Adaptation" has to be carried out until the same "tube dependent" value appears.

Select the next Focus, if necessary and carry out the above mentioned procedure.

Close the adaption procedure by selecting

/ End adjust/ in the TCOP menu.

Now the system is in

Application Mode.

Remark:

If the two last values of the Boost Adaptation are not equal, carry out the adaption again.