Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00XT | Error/Warning |
Description:
Rotation in CU and FU_RC high speed or FU_CIE for low speed different.
Possible Causes / Advice:
If more than 4 PREP's have been switched within one minute the 5th will cause this entry not allowing the next acceleration to prevent overheating of the stator. Bouncing handswitch? Check behavior at EN_X/ EZX82 and compare with the normal sample waveform. If in combination with 10LA (FU_RC high speed only) program "enable" at "rotation prolongation after prep".