## FU - kV measure temperatures

##### Monitoring |  |  |  |
Measure Temperatures |  |  |
tube temp switch: |  | short circuit (against ground) = red traffic light on at control desk closed = normal condition, green traffic light on at control desk open = open cable connection / tube too hot, red traffic light at control desk
tube sensor [ ‘C]: |  | not yet available, ignore
converter 1 [ ‘C]: |  | range without warning 0ºC...85ºC
converter 2 [ ‘C]: |  | range without warning 0ºC...85ºC only with 65/80kW with 50kW versions -273ºC (line open)
ht-tank [ ‘C] : |  | range without warning 0ºC...80ºC