Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
10TD | Error |
Description:
invalid data for tube %u
Possible Causes / Advice:
Appears most likely after exchange of high speed rotor control unit to version 4512 104 71421/61 which requires the new data for the RC firmware, tube file TUBE_R3 (use version file date 18.4.2001). Reload tube data using XRGSCOPE R3. Appears with a non-programmed CU after the very first turn-on. When appearing after CU Complete restore the data file might be defective. Dump CU Complete file which doesn't work, upload CU Complete again, using the following procedure. PC Up/Download Procedure. If the error is permanent erase NV-RAM and start programming from scratch. Memory Quick Erase Procedure