### Options

This screen displays all options programmed in the function key EZ139 D38 (compare with STAMMKARTE at the cover of the frontal kV converter and add-on STAMMKARTE updates).

example:

Power Class (kW): [ xx ] xx = 50 / 65 / 80 possible

*****: [yes/no] not used

RF: [yes/no] Optimus R/F hardware, all Bucky functions possible

Bucky: [yes/no] Optimus RAD hardware, no fluoro or fluoro upgrade possible

TDC: [yes/no] tomo density control

AEC: [yes/no] automatic exposure control

APR disabled: [yes/no] yes = no APR visible at control desk

*****: [yes/no] not used

*****: [yes/no] not used

*****: [yes/no] not used

Vario Focus: [yes/no] only RO16/48, RO17/50, SRO09/51, SRO25/50, SRO33/100

External Tomo Time: [yes/no] via system CAN or WA units

OEM: [yes/no] not used

Area Exposure Product: [yes/no] only with Galileo collimator

Tube Protection: [yes/no] if no exposures can be switched with red tube heat indicator

on, overload exposure counter active

PDO: [yes/no] patient data organizer

*****: [yes/no] not used