Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
03AC | Warning |
Description:
Emission current (Ie) regulation active on two filaments
Possible Causes / Advice:
Under normal conditions only one focus is active during exposure and fluoroscopy, the second focus is in standby. Exception: Variofocus The small focus filament current is always constant, the additional part of the emission current Variofocus will be controlled by the large focus.