This tool is very helpful to see if there are some signals on the signalbus missing.

It is a quick way to check if the signals are reaching the OMTC_TheBox Generator, coming from the System Controller.

EN_X = enable X-ray

NR_PR_X = not ready preparing for X-ray

RQ_SN_X = request synchronization of X-ray, system level

CTRL_X = control X-ray request command, system level

CTRL_X_C = control X-ray request command, internal generator level

X_ACT_S = X-ray active signal, kV >75% nominal value (old= HTON)

RQ_PH_X =

RQ_PL_X =

RQ_CO_X =