Important!

In case of downgrading MRC type to e.g. MRM type:

1. First deselect the MRC tube type by selecting: empty string

2. Disconnect the tube physically

3. Install the new MRM tube

4. Configure the required MRM tube in this menu

Mains Data:

Fill in the nominal mains voltage between 380V and 480V

Any value in between is possible.

Mains resistance:

Fill in the measured value.

For the maximum value refer to the documentation, chapter "Technical Data"

Limit kV:

Only the value is displayed, you filled in during the tube conditioning.

Cable type:

The cable type and capacity [pf/m] is mentioned in the cable documentation.

Cable length:

You can read the cable length from the codenumber on the HT plug e.g.

9806 402 6xx02 xx = cable length

Prefilter:

It depends on the collimator you have installed in the system.