### Bucky/Scopo 1WB

#### Bucky RGDV:

Eight RGDV’s can be programmed at the same system ready contact WBX11 pins 9-10
(R/F controller, ready = closed).
Activates also the format size correction contact (closed if > 24x24 cm) WB X11 pins 1-2 (Bucky chambers only).

if no automatic collimator exists, insert a link at pins 1-2 to get access to the side field selection (Bucky chambers only) if no Bucky Ready contact exists, but the format size correction has to be active: insert a link at WBX11 pins 9-10 (Bucky chambers only)