### SW/HW – Versions

This screen displays the actual firmware versions Release, Version (don’t care) and Level.

For PCB Central Unit it also displays the hardware version
(must be 2 for Optimus RAD/RF Rel. 3.x or Optimus C Rel. 1.x).

CU APPL SW: | [R3V1L5] | 4512 114 20835 |
CU BOOT SW: | [R3V1L1] | 4512 113 20731 |
FU kV: | [R3V1L2] | 4512 113 20132 | as an example for Optimus RAD
FU mA a: | [R1V1L2] | 4512 113 20212 |
FU mA b: | [ - - - - - ] |  |
FU mA c: | [ - - - - - ] |  |
FU mA d: | [ - - - - - ] |  |
FU CIE: | [R1V1L1] | 4512 113 20311 | as standard version
FU HI a: | [R2V1L5] | 4512 113 20525 |
FU HI b: | [ - - - - - ] |  |
FU RC a: | [R2V1L3] | 4512 113 22323 | with the new RoCo 4512 104 71421/461
FU RC b: | [ - - - - - ] |  |
FU RC c: | [ - - - - - ] |  |
FU AD a(1WA): | [R1V1L1] | 4512 113 20611 |
FU AD b(2WA): | [R1V1L1] | 4512 113 20611 |
FU AD c(1WB): | [R1V1L1] | 4512 113 20611 |
FU AD d(2WB): | [ - - - - - ] |  |
FU MDO: | [ - - - - - ] |  |
CU HW: | [ 2 ] |  |