Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00PL | Error/Warning |
Description:
CPU: dose digits disturbance Noise level at chamber signal input increases a limit value before kV is started.
Possible Causes / Advice:
Check signal waveform in standby, prep and ready 2 condition before the exposure starts. The chamber signal at EZ150 X4 should not be greater than the values listed below. Otherwise the problem source has to be investigated. > 20mV release 3.3 > 80mV release 3.5 This error is solved in R3.5 SW with FCO 74200002. This FCO is "Retrofit on Failure" so it will not automatically come to the site. Does not exist at release 2.x generators.