### CAN Auto Configuration

(not required for Optimus C)

Start function: Update Generator Config:

<OK> gives the command for CU to scan on the internal generator CAN bus and update the generator CAN member list (assign units on the list).

Minimum configuration of an OPTIMUS (see also ‘Faultfind -Power ON Results - Internal CAN Configuration’:

FU_mA (EZ119), FU_kV (EZ130), FU_CU (EZ139), FU_CIE (EZ150) FU_RC_a (EY100).

Other units are not applicable for DUO DIAGNOST.

CU updates the member list during the very first turn-on by itself.

<CANCEL> or <ESC> nothing changes