### Tube 1...3 Speed Selection

range = 3000...9000 rpm

#### Exposure rotation [RPM]:

Fast Exposure rotation [RPM]: (fast exposure not applicable for Optimus R/F)

Fluoroscopy rotation [RPM]: fluoroscopy without rotation is not possible

The speed for the tube type and technique is automatically taken from the tube data file.

Fluoroscopy without rotation is not possible.

All stators have to be connected as an SRO tube, see doc INSTALLATION