Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00L4 | Error/Warning |
Description:
GC: limits inconsistent During service work online with the PC such error might come up after whatever XRGSCOPE screen has been sent with <F2> to the generator.
Possible Causes / Advice:
Check RGDV Data Set B "Tube power factor [%]: ": If [***] appears set [100] instead, check all other Data Set B settings as they might have changed too.