Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
DR_TV_PO
Dose rate of TV chain signal positive, fluoro control (II/TV_adapter_PCB_X3:3-X2:7) - EZX61:7 - EZ139X2:A19 backpanel version 4512 108 09361/2 -/+12V positive polarity dual voltage differential signal typically -6V in standby coming from TV chain -V for more dose, +V for less dose, 0V stable image part of: dose rate control