Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
03BA | Warning |
Description:
Coordinates not monotonous; boost adaptation error
Possible Causes / Advice:
With PC and XRGSCOPE: Select Unit > FU-mA > FU-mA > Faultfind > Adaptation Results > Select Adaptation Table for Reading Type in at focus: 1 = large focus tube 1 2 = small focus tube 1 Type in a kV value between min and max or if known the kV value at which the generator errors. > Read Previously Selected Adaptation Table detailed explanations see If-Ie Data Table. Use firmware of FU_mA version 4512 113 20212 if previous version installed.