Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HW | Warning |
Description:
kV anode out of range, asymmetrical : ±15% 2 detections within 20 ms
Possible Causes / Advice:
Connect an oscilloscope to EZ130 X1:C17 (HT_AN ) and EZ130 X1:C16 (HT_CA) (10KV/V)and monitor the KV waveform at the input to the EZ130. Trigger = EZX74 (CTRL_X_C) OR Connect an oscilloscope to EZ130:X3 (AV_HT_AN ) and EZ130:X4 (AV_HT_CA) (20KV/V)and monitor the KV waveform at the output of the EZ130.Trigger = EZX74 (CTRL_X_C) Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15