Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00TG | Error |
Description:
TTS (Tube Temperature Supervision): Tube overheated
Possible Causes / Advice:
The mA measuring circuit might be defective, check circuit in standby against oscilloscope screenshot ma_pulse.pcx most likely in non-AEC technique. Wrong calculation of switched loads. Exchange high tension transformer. Exchange FU_mA PROM by version 4512 113 20212. Check if application data (APR, system dependent) can be improved.