Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HQ | Warning |
Description:
High tension tank temperature out of range: 0 C > T > 80 C 3 detections within 30 ms
Possible Causes / Advice:
4.4V...1.5V = 20...100 deg C at EZ130 X1:C19 Measured with NTC resistor 15kOhms (+/-10%, 20 deg C) Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PCB.