Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HG | Warning |
Description:
kV actual value out of range +/- (4% +1kV) 2 measurements within 20ms
Possible Causes / Advice:
If this error occurs in combination with 02WK, 02HH, & 00XO see Service Recommendation 00 135 015 With a PC and XRGSCOPE: select error # from error log index list, select error details and read screen Error: HW Set Values to get KV nominal, then read Error: Read HW Values to get the faulty value. Monitor with oscilloscope at EZ130 X3 AVHT 20kV/V or X4 (anode) and X5 (cathode). trigger: CTRL_X_C/ EZX74 Release 2 generators: Check kV behavior against document kV1_2_mod.doc and carry out modification if necessary. Carry out kV driver test chapter 8.2 FAULT FINDING Release 3 generators: Check and carry out adjustment "factor for duty" cycle according to document adj_duty_cycle_factor.doc Carry out kV driver test chapter 5.3 register Converter R/F Check if FCO 00 135 014 has been carried out All Generators Check Mains conditions. Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PCB.