## FU - mA read actual status

##### Read Actual Status |  | Gives the actual status of the filament circuit. Several entries are possible in the three fields.
foc | = | see table (‘focus number FU-mA’)
static | = | condition of the filament like: FOCini no tube programmed normal tube programmed and adapted
dynamic | = | actual dynamic condition like: off - no tube programmed single focus tube, this circuit not in use standby in standby without error ctrl Xray during exposure or fluoro