Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00BU | Error/Warning |
Description:
Adaptation paused due to missing load
Possible Causes / Advice:
If the tube temperature supervision sees any of the temperatures beyond a limit to allow 100% load adaptation waits until a 100% load is possible and keeps on automatically. 00BU will not be displayed at the control desk or on the service PC, the only indication is the red traffic light at the control desk and a flickering "Waiting" window on the PC screen