Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
EN_X/
Enable X-ray, system level preparation or fluoro request, only valid in combination with CAN message (RAD-R/F) or hardware requests (Optimus C) EZ139X1:C2 - EZX10:1/3 - EZX23:15-EZX45:11 - EZX46:11 - C300X1:11 - EWAX51:11 - EWAX52:11 - EWA100X2:C26 - EWBX51:11 - EWBX52:11 - EWB100X2:C26 measuring point: EZX82, EZ139X9 part of: signal bus 0V/+15V low active