### Tube 1...3 Data Set

Note!

The tube firmware TUBE_R3.TDL (18.4.2001 or newer) is required to drive the new version of rotor control 4512 104 7142x or 4512 104 7146x with firmware 4512 113 22322/3.

It also runs on all predecessor rotor controls 4512 104 71401...6 with firmware 4512 113 22312.

#### Function:

- After ~ 35 sec of Reading (spinning bar) the screen Load Data from Disk comes up offering the default TUBE_R3.TDL. file
- With <OK> a screen Available Tubes (Rel.3 Format) offers a selection of all available tubes in non-cooled housings ROT350 (250W) or water cooled housings ROT351 (450W).
- After tube selection a screen Analyzing will come up, followed by Transmitting and then Percent transmitted (how much of file has been loaded to the generator).

#### Attentation:

- Wait until the PC comes up with the message

# Programming the tube might require the tube load counter to be reset <OK>

- followed by a message to reset the generator.

!! D O N O T R E S E T B E F O R E !!

- For single focus tubes like RO30:

All APR's must get the large focus programmed.

#### Tube exchange:

Do not forget to carry out the 'Reset Tube Statistic' command.