Carry out this procedure for all FSC used in the system. (0....5)

Make a standard AEC exposure.

Measure the density of the developed film.

Fill in the requested dose and the measured dose. The calculated result is displayed in the "Value [%]" field.

The result is calculated by using the following formule:

((requested optical density) / (measured optical density)) X 100 [%]

You can also fill in the switch off dose in the "Value[%]" field manually without using automatic calculation.