Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
RM_DR_0V
Room door contact 0V EZ150X1:C28 - EZX1:10 - EWGX1:10 - EWGX2:10 - EWGX3:10 release 2 generators only, not used release 3 RAD-R/F and Optimus C partner of RM_DR_CT signal release 2 RAD generators only 0V/+26V low active, detects room door contact signal short circuit at release 2 RAD generators during turn-on