### Fluoroscopy Curves

20 Fluoroscopy curve memories can be loaded with one of the 3 predefined fluoro curves of the installation disk file FLUOCURV.TDL:

default curves FLUOCURV.TDL | start values 50 kV | kV-mA characteristic
40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | kV
6mA default 1 | 0.5 mA | 0.25 | 0.5 | 0.95 | 1.7 | 3.0 | 5.0 | 5.5 | 6.0 | mA
6mA default 2 | 0.4 mA | 0.25 | 0.4 | 0.6 | 0.8 | 2.0 | 4.0 | 5.0 | 6.0 | mA
3mA | 0.5 mA | 0.22 | 0.42 | 0.7 | 1.2 | 2.15 | 2.7 | 2.95 | 3.0 | mA

One out of the programmed curves (1...20) has to be attached to the APR data set,

see ‘Change APR’.

If other curves for special applications are required, send a request to Helpdesk Hamburg.