### Area Exposure Product

Displayed at the control desk only if option (9890 000 0256x, see STAMMKARTE) present (see ‘Faultfind - Power ON Results - Options’) with GALILEO collimator if ‘Bucky Ctrl. 1/Dig. Diag.’ or ‘Thoravision’ set.

TH + TH2: Dose value display of all exposures of a patient, must be reset with next patient.
Thoravision: The dose value is not displayed at the control desk, as the system controller
takes the value and resets the value afterwards with the command next patient. The dose value will be displayed on the images.
Digital Diagnost: The dose value of the last exposure will remain on the desk until the next exposure will be started.

#### Specific Yield of Tube 1...3

Procedure to measure and modify the specific tube yield see doc ADJUSTMENTS. The default yield data table is on the installation disk: RE_YIEL.TDL.