Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
03HH | Error |
Description:
Filament current (If) setpoint too large
Possible Causes / Advice:
.With a PC and XRGSCOPE: Select error # from error log index list, select error details, and read screen Error: Read HW Values to get the setpoint and the faulty value. If error is persistent go path: > Select Unit > FU-mA > FU-mA > Faultfind > Monitoring > read If nominal fil. circuit 1 = small focus fil. circuit 2 = large focus Check supply voltages EZ119 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PC