Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
CU Complete PC settings
Optimus RAD-R/F release 2.x and 3.x CMOS data are up-/downloaded in one string without handshake. Any kind of interruption can cause the loading process to fail. Problems occur mainly during the download to the PC. A download file which is not complete can not be used as safety backup file. The service PC can be prepared to guarantee a safe loading process. XRGSCOPE should be started from DOS if possible. No screensaver should be active. No other program, application or CD drive should be active using WINDOWS any version. Any kind of power management of the PC hardware as well as the WINDOWS power management should be off. If connected to mains power some of these might be automatically off. Preparing the generator: At generators which are connected to a system with CAN connected controller the CAN connection EZX43-1 or EZX42-1 + 43-1 must be removed. Thoravision Bucky TH + TH2 Digital Diagnost Easy Diagnost systems with Bucky unit The signal bus EZX23 must also be removed with the following systems. Thoravision Digital Diagnost Then the generator has to be turned on. The download procedure must not be started before ENK1 energized about 2 minutes after turn-on. At generators with a non-CAN system the loading process can be started once ENK1 energized. CU Complete download files and other xxx.TDL files should be mailed in a zipped format. xxx.TDL files are ASCII files which might be "modified" during mailing.