Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
07LJ | Error |
Description:
RC Maximal rotation time exceeded
Possible Causes / Advice:
Maximal rotation time low speed rotor control exceeded FU_CIE time out if preparation still active after 60 seconds, exposure ready disappears after max free run time 30 seconds. During adaptation if in site with Bucky TH system BuCo release 5.x which does not allow an exposure repetition, change settings free cassette RGDV. See Adaption Procedure.