Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
03PF | Error |
Description:
No kV discharged due to missing emission current
Possible Causes / Advice:
Conditioning procedures must never be carried out with the small filaments. Installation: HT cables anode and cathode side interchanged at one side? Short circuit in HT cable for selected focus.Filament short circuit, possibly in combination with 03PA.