Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
STV
Stator phase V = common EYAX2:3 - EX1102 low speed rotor control single tube EYAX2:3 - EWGK11:3 - EWGK12:3=EWGK11:4=EWGK12:4 low speed two tubes EY100X47:1 - EX1102 high speed rotor control versions 4512 104 33791/2 or 71401..6 single tube EY100X47:1 - EWGK11:3 - EWGK12:3=EWGK11:4=EWGK12:4 high speed rotor control versions 4512 104 33791/2 or 71401..6 two tubes EY100X52 - EX1102 high speed rotor control version 4512 104 71421/61 single tube EY100X52 -- EWGK11:3 - EWGK12:3=EWGK11:4=EWGK12:4 high speed rotor control version 4512 104 71421/61 two tubes